    1. POWERTRAIN CODES • P0016 - Crankshaft Position Camshaft Position Correlation Bank 1 Sensor A • P0030 - Heated Oxygen Sensor (H02S) Heater Control Circuit Bank 1 Sensor 1 • P0031 - Heated Oxygen Sensor (HO2S) Heater Circuit Low Voltage Bank 1 Sensor 1 • P0032 - Heated Oxygen Sensor (HO2S) Heater Circuit High Voltage Bank 1 Sensor 1 • P0036 - Heated Oxygen Sensor (HO2S) Heater Control Circuit Bank 1 Sensor 2 • P0037 - Heated Oxygen Sensor (HO2S) Heater Circuit Low Voltage Bank 1 Sensor 2 • P0038 - Heated Oxygen Sensor (HO2S) Heater Circuit High Voltage Bank 1 Sensor 2 • P0050 - Heated Oxygen Sensor (HO2S) Heater Circuit Bank 2 Sensor 1 • P0051 - Heated Oxygen Sensor (HO2S) Heater Circuit Low Voltage Bank 2 Sensor 1 • P0052 - Heated Oxygen Sensor (HO2S) Heater Circuit High Voltage Bank 2 Sensor 1 • P0053 - HO2S Heater Resistance Bank 1 Sensor 1 (PCM) • P0054 - HO2S Heater Resistance Bank 1 Sensor 2 (PCM) • P0056 - Heated Oxygen Sensor (HO2S) Heater Circuit Bank 2 Sensor 2 • P0057 - Heated Oxygen Sensor (HO2S) Heater Circuit Low Voltage Bank 2 Sensor 2 • P0058 - Heated Oxygen Sensor (HO2S) Heater Circuit High Voltage Bank 2 Sensor 2 • P0068 - Throttle Body Airflow Performance (PCM) • P0100 - MAF Sensor Circuito Insuficiente Activita • P0101 - Mass Air Flow (MAF) Sensor Performance • P0102 - Mass Air Flow (MAF) Sensor Circuit Low Frequency • P0103 - Mass Air Flow (MAF) Sensor Circuit High Frequency • P0104 - Mass Air Flow Circuit Intermittent • P0105 - MAP Sensor Circuito Insuficiente Activita • P0106 - Manifold Absolute Pressure (MAP) System Performance • P0107 - Manifold Absolute Pressure (MAP) Sensor Circuit Low Voltage • P0108 - Manifold Absolute Pressure (MAP) Sensor Circuit High Voltage • P0109 - Manifold Absolute Pressure Circuit Intermittent • P0110 - Intake Air Temperature (IAT) Sensor Circuit • P0111 - Intake Air Temperature (IAT) Sensor Performance • P0112 - Intake Air Temperature (IAT) Sensor Circuit Low Voltage • P0113 - Intake Air Temperature (IAT) Sensor Circuit High Voltage • P0114 - Intake Air Temperature Circuit Intermittent • P0115 - Engine Coolant Temperature (ECT) Sensor Circuit • P0116 - Engine Coolant Temperature (ECT) Sensor Performance • P0117 - Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage
    2. • P0118 - Engine Coolant Temperature (ECT) Sensor Circuit High Voltage • P0119 - Engine Coolant Temperature Circuit Intermittent • P0120 - TP System Performance • P0121 - TP Sensor Circuit Insufficient Activity • P0122 - Throttle Position (TP) Sensor Circuit Low Voltage • P0123 - Throttle Position (TP) Sensor Circuit High Voltage • P0124 - Throttle Position Sensor 1 Circuit Intermittent • P0125 - Engine Coolant Temperature (ECT) Insufficient for Closed Loop Fuel Control • P0126 - Insufficient ECT for Stable Operation • P0128 - Coolant Thermostat Below Thermostat Regulating Temperature • P0130 - Heated Oxygen Sensor (HO2S) Circuit Closed Loop (CL) Performance Bank 1 Sensor 1 • P0131 - Heated Oxygen Sensor (HO2S) Circuit Low Voltage Bank 1 Sensor 1 • P0132 - Heated Oxygen Sensor (HO2S) Circuit High Voltage Bank 1 Sensor 1 • P0133 - Heated Oxygen Sensor (HO2S) Slow Response Bank 1 Sensor 1 • P0134 - Heated Oxygen Sensor (HO2S) Circuit Insufficient Activity Bank 1 Sensor 1 • P0135 - Heated Oxygen Sensor (HO2S) Heater Performance Bank 1 Sensor 1 • P0136 - Heated Oxygen Sensor (HO2S) Circuit Bank 1 Sensor 2 • P0137 - Heated Oxygen Sensor (HO2S) Circuit Low Voltage Bank 1 Sensor 2 • P0138 - Heated Oxygen Sensor (HO2S) Circuit High Voltage Bank 1 Sensor 2 • P0139 - Heated Oxygen Sensor (HO2S) Slow Response Bank 1 Sensor 2 • P0140 - Heated Oxygen Sensor (HO2S) Circuit Insufficient Activity Bank 1 Sensor 2 • P0141 - Heated Oxygen Sensor (HO2S) Heater Performance Bank 1 Sensor 2 • P0142 - Heated Oxygen Sensor (HO2S) Circuit Bank 1 Sensor 3 • P0143 - Heated Oxygen Sensor (HO2S) Circuit Low Voltage Bank 1 Sensor 3 • P0144 - Heated Oxygen Sensor (HO2S) Circuit High Voltage Bank 1 Sensor 3 • P0145 - Heated Oxygen Sensor (HO2S) Circuit Bank 1 Sensor 2 Slow Response • P0146 - Heated Oxygen Sensor (HO2S) Circuit Insufficient Activity Bank 1 Sensor 3 • P0147 - Heated Oxygen Sensor (HO2S) Heater Performance Bank 1 Sensor 3 • P0150 - Heated Oxygen Sensor (HO2S) Circuit Closed Loop (CL) Performance Bank 2 Sensor 1 • P0151 - Heated Oxygen Sensor (HO2S) Circuit Low Voltage Bank 2 Sensor 1 • P0152 - Heated Oxygen Sensor (HO2S) Circuit High Voltage Bank 2 Sensor 1 • P0153 - Heated Oxygen Sensor (HO2S) Slow Response Bank 2 Sensor 1 • P0154 - Heated Oxygen Sensor (HO2S) Circuit Insufficient Activity Bank 2 Sensor 1 • P0155 - Heated Oxygen Sensor (HO2S) Heater Performance Bank 2 Sensor 1 • P0156 - Heated Oxygen Sensor (HO2S) Circuit Bank 2 Sensor 2 • P0157 - Heated Oxygen Sensor (HO2S) Circuit Low Voltage Bank 2 Sensor 2 • P0158 - Heated Oxygen Sensor (HO2S) Circuit High Voltage Bank 2 Sensor 2
    3. • P0159 - Heated Oxygen Sensor (HO2S) Slow Response Bank 2 Sensor 2 • P0160 - Heated Oxygen Sensor (HO2S) Circuit Insufficient Activity Bank 2 Sensor 2 • P0161 - Heated Oxygen Sensor (HO2S) Heater Performance Bank 2 Sensor 2 • P0162 - Heated Oxygen Sensor (HO2S) Circuit Bank 2 Sensor 3 • P0163 - Heated Oxygen Sensor (HO2S) Circuit Bank 2 Sensor 3 Low Voltage • P0164 - Heated Oxygen Sensor (HO2S) Circuit Bank 2 Sensor 3 High Voltage • P0165 - Heated Oxygen Sensor (HO2S) Circuit Bank 2 Sensor 3 Slow Response • P0166 - Heated Oxygen Sensor (HO2S) Circuit Bank 2 Sensor 3 No Activity Detected • P0167 - Heated Oxygen Sensor (HO2S) Heater Circuit Bank 2 Sensor 3 • P0169 - Fuel Composition Sensor • P0170 - Fuel Trim Bank 1 • P0171 - Fuel Trim System Lean Bank 1 • P0172 - Fuel Trim System Rich Bank 1 • P0173 - Fuel Trim Bank 2 • P0174 - Fuel Trim System Lean Bank 2 • P0175 - Fuel Trim System Rich Bank 2 • P0176 - Fuel Composition Sensor Circuit • P0177 - Fuel Composition Sensor Circuit Performance • P0178 - Fuel Composition Sensor Circuit Low Voltage • P0179 - Fuel Composition Sensor Circuit High Voltage • P0180 - Fuel Temperature Sensor 1 Circuit • P0181 - Fuel Temp. Sensor 1 Circuit Performance • P0182 - Fuel Temperature Sensor Circuit Low Voltage • P0183 - Fuel Temperature Sensor Circuit High Voltage • P0184 - Fuel Temperature Sensor 1 Circuit Intermittent • P0185 - Fuel Temperature Sensor 2 Circuit • P0186 - Fuel Temp. Sensor 2 Circuit Performance • P0187 - Fuel Temperature Sensor 2 Circuit Low Voltage • P0188 - Fuel Temperature Sensor 2 Circuit High Voltage • P0189 - Fuel Temperature Sensor 2 Circuit Intermittent • P0190 - Fuel Rail Pressure Sensor Circuit • P0191 - Fuel Rail Pressure Sensor Circuit Performance • P0192 - Fuel Rail Pressure Sensor Circuit Low Voltage • P0193 - Fuel Rail Pressure Sensor Circuit High Voltage • P0194 - Fuel Rail Pressure Sensor Circuit Intermittent • P0195 - Engine Oil Temperature Sensor • P0196 - Engine Oil Temperature Sensor Performance • P0197 - Engine Oil Temperature Sensor Low Voltage • P0198 - Engine Oil Temperature Sensor High Voltage • P0199 - Engine Oil Temperature Sensor Intermittent • P0200 - Injector Control Circuit • P0201 - Injector 1 Control Circuit
    4. • P0202 - Injector 2 Control Circuit • P0203 - Injector 3 Control Circuit • P0204 - Injector 4 Control Circuit • P0205 - Injector 5 Control Circuit • P0206 - Injector 6 Control Circuit • P0207 - Injector 7 Control Circuit • P0208 - Injector 8 Control Circuit • P0209 - Injector 9 Control Circuit • P0210 - Injector 10 Control Circuit • P0211 - Injector 11 Control Circuit • P0212 - Injector 12 Control Circuit • P0213 - Cold Start Injector 1 • P0214 - Cold Start Injector 2 • P0215 - Engine Shutoff Control Circuit • P0216 - Injection Timing Control Circuit • P0217 - Engine Overtemp Condition • P0218 - Transmission Fluid Overtemperature • P0219 - Engine Overspeed Condition • P0220 - APP Sensor 2 Circuit • P0221 - APP (Throttle Position) Sensor 2 Circuit Performance • P0222 - APP (Throttle Position) Sensor 2 Circuit Low Voltage • P0223 - APP (Throttle Position) Sensor 2 Circuit High Voltage • P0224 - Throttle Position Sensor 2 Intermittent • P0225 - APP Sensor 3 Circuit • P0226 - APP Sensor 3 Circuit Performance • P0227 - APP Sensor 3 Circuit Low Voltage • P0228 - APP Sensor 3 Circuit High Voltage • P0229 - Throttle Position Sensor 3 Intermittent • P0230 - Fuel Pump Relay Control Circuit • P0231 - Fuel Pump Feedback Circuit Low Voltage • P0232 - Fuel Pump Feedback Circuit High Voltage • P0233 - Fuel Pump Secondary Circuit Intermittent • P0234 - Turbocharger Engine Overboost Condition • P0235 - Turbocharger Boost Sensor 1 Circuit • P0236 - Turbocharger Boost System • P0237 - Turbocharger Boost Sensor Circuit Low Voltage • P0238 - Turbocharger Boost Sensor Circuit High Voltage • P0239 - Turbocharger Boost Sensor 2 Circuit • P0240 - Turbocharger Boost Sensor 2 Performance • P0241 - Turbocharger Boost Sensor 2 Circuit Low Voltage • P0242 - Turbocharger Boost Sensor 2 Circuit High Voltage • P0243 - Turbocharger Wastegate Solenoid 1 • P0244 - Turbocharger Wastegate Solenoid 1 Performance • P0245 - Turbocharger Wastegate Solenoid 1 Low Voltage • P0246 - Turbocharger Wastegate Solenoid 1 High Voltage
    5. • P0247 - Turbocharger Wastegate Solenoid 2 • P0248 - Turbocharger Wastegate Solenoid 2 Performance • P0249 - Turbocharger Wastegate Solenoid 2 Low Voltage • P0250 - Turbocharger Wastegate Solenoid 2 High Voltage • P0251 - Injection Pump Fuel Metering Control "A" Malfunction (Cam/Rotor/Injector) • P0252 - Injection Pump Fuel Metering Control "A" Range/Performance (Cam/Rotor/Injector) • P0253 - Injection Pump Fuel Metering Control "A" Low (Cam/Rotor/Injector) • P0254 - Injection Pump Fuel Metering Control "A" High (Cam/Rotor/Injector) • P0255 - Injection Pump Fuel Metering Control "A" Intermittent (Cam/Rotor/Injector) • P0256 - Injection Pump Fuel Metering Control "B" Malfunction (Cam/Rotor/Injector) • P0257 - Injection Pump Fuel Metering Control "B" Range/Performance (Cam/Rotor/Injector) • P0258 - Injection Pump Fuel Metering Control "B" Low (Cam/Rotor/Injector) • P0259 - Injection Pump Fuel Metering Control "B" High (Cam/Rotor/Injector) • P0260 - Injection Pump Fuel Metering Control "B" Intermittent (Cam/Rotor/Injector) • P0261 - Cylinder 1 Injector Circuit Low • P0262 - Cylinder 1 Injector Circuit High • P0263 - Cylinder 1 Contribution/Balance Fault • P0264 - Cylinder 2 Injector Circuit Low • P0265 - Cylinder 2 Injector Circuit High • P0266 - Cylinder 2 Contribution/Balance Fault • P0267 - Cylinder 3 Injector Circuit Low • P0268 - Cylinder 3 Injector Circuit High • P0269 - Cylinder 3 Contribution/Balance Fault • P0270 - Cylinder 4 Injector Circuit Low • P0271 - Cylinder 4 Injector Circuit High • P0272 - Cylinder 4 Contribution/Balance Fault • P0273 - Cylinder 5 Injector Circuit Low • P0274 - Cylinder 5 Injector Circuit High • P0275 - Cylinder 5 Contribution/Balance Fault • P0276 - Cylinder 6 Injector Circuit Low • P0277 - Cylinder 6 Injector Circuit High • P0278 - Cylinder 6 Contribution/Balance Fault • P0279 - Cylinder 7 Injector Circuit Low • P0280 - Cylinder 7 Injector Circuit High • P0281 - Cylinder 7 Contribution/Balance Fault • P0282 - Cylinder 8 Injector Circuit Low • P0283 - Cylinder 8 Injector Circuit High • P0284 - Cylinder 8 Contribution/Balance Fault • P0285 - Cylinder 9 Injector Circuit Low
    6. • P0286 - Cylinder 9 Injector Circuit High • P0287 - Cylinder 9 Contribution/Balance Fault • P0288 - Cylinder 10 Injector Circuit Low • P0289 - Cylinder 10 Injector Circuit High • P0290 - Cylinder 10 Contribution/Balance Fault • P0291 - Cylinder 11 Injector Circuit Low • P0292 - Cylinder 11 Injector Circuit High • P0293 - Cylinder 11 Contribution/Balance Fault • P0294 - Cylinder 12 Injector Circuit Low • P0295 - Cylinder 12 Injector Circuit High • P0296 - Cylinder 12 Contribution/Range Fault • P0300 - Engine Misfire Detected • P0301 - Cylinder 1 Misfire Detected • P0302 - Cylinder 2 Misfire Detected • P0303 - Cylinder 3 Misfire Detected • P0304 - Cylinder 4 Misfire Detected • P0305 - Cylinder 5 Misfire Detected • P0306 - Cylinder 6 Misfire Detected • P0307 - Cylinder 7 Misfire Detected • P0308 - Cylinder 8 Misfire Detected • P0309 - Cylinder 9 Misfire Detected • P0310 - Cylinder 10 Misfire Detected • P0311 - Cylinder 11 Misfire Detected • P0312 - Cylinder 12 Misfire Detected • P0313 - Misfire Detected With Low Fuel Level • P0315 - Crankshaft position (CKP) system variation values are not stored in the PCM memory • P0318 - Rough Road Sensor Circuit • P0320 - Ignition/Distributor Engine Speed Input Circuit Malfunction • P0321 - Ignition/Distributor Engine Speed Input Circuit Range/Performance • P0322 - IC Module 4X Reference Circuit No Frequency • P0323 - Ignition/Distributor Engine Speed Input Circuit Intermittent • P0324 - Knock Sensor (KS) Module Performance • P0325 - PCM Knock Sensor Circuit • P0326 - Knock Sensor Circuit Excessive Spark Retard • P0327 - Knock Sensor Circuit Low Voltage • P0328 - Knock Sensor 1 Circuit High Input (Bank 1 or Single Sensor) • P0329 - Knock Sensor 1 Circuit Intermittent (Bank 1 or Single Sensor) • P0330 - Knock Sensor (KS) Circuit Bank 2 • P0331 - Knock Sensor 2 Circuit Range/Performance (Bank 2) • P0332 - Knock Sensor 2 Circuit Low Input (Bank 2) • P0333 - Knock Sensor 2 Circuit High Input (Bank 2) • P0334 - Knock Sensor 2 Circuit Intermittent (Bank 2) • P0335 - CKP Sensor A Circuit Performance • P0336 - Crankshaft Position (CKP) Sensor A Performance
    7. • P0337 - Crankshaft Position (CKP) Sensor Circuit Low Duty Cycle • P0338 - Crankshaft Position (CKP) Sensor Circuit High Duty Cycle • P0339 - Crankshaft Position (CKP) Sensor Circuit Intermittent • P0340 - Camshaft Position (CMP) Sensor Circuit • P0341 - Camshaft Position (CMP) Sensor Performance • P0342 - Camshaft Position Sensor Circuit Low Input • P0343 - Camshaft Position Sensor Circuit High Input • P0344 - Camshaft Position Sensor Circuit Intermittent • P0350 - Ignition Coil Primary/Secondary Circuit Malfunction • P0351 - Ignition Coil 1 Control Circuit • P0352 - Ignition Coil 2 Control Circuit • P0353 - Ignition Coil 3 Control Circuit • P0354 - Ignition Coil 4 Control Circuit • P0355 - Ignition Coil 5 Control Circuit • P0356 - Ignition Coil 6 Control Circuit • P0357 - Ignition Coil 7 Control Circuit • P0358 - Ignition Coil 8 Control Circuit • P0359 - Ignition Coil I Primary/Secondary Circuit Malfunction • P0360 - Ignition Coil J Primary/Secondary Circuit Malfunction • P0361 - Ignition Coil K Primary/Secondary Circuit Malfunction • P0362 - Ignition Coil L Primary/Secondary Circuit Malfunction • P0370 - Timing Reference High Resolution Signal A Malfunction • P0371 - IC 24X Reference Circuit Too Many Pulses • P0372 - IC 24X Reference Circuit Missing Pulses • P0373 - Timing Reference High Resolution Signal A Intermittent/Erratic Pulses • P0374 - Timing Reference High Resolution Signal A No Pulses • P0375 - Timing Reference High Resolution Signal B Malfunction • P0376 - Timing Reference High Resolution Signal B Too Many Pulses • P0377 - Timing Reference High Resolution Signal B Too Few Pulses • P0378 - Timing Reference High Resolution Signal B Intermittent/Erratic Pulses • P0379 - Timing Reference High Resolution Signal B No Pulses • P0380 - Glow Plug/Heater Circuit "A" Malfunction • P0381 - Glow Plug/Heater Indicator Circuit Malfunction • P0382 - Exhaust Gas Recirculation Flow Malfunction • P0385 - Crankshaft Position (CKP) Sensor B Circuit • P0386 - Crankshaft Position (CKP) Sensor B Performance • P0387 - Crankshaft Position Sensor B Circuit Low Input • P0388 - Crankshaft Position Sensor B Circuit High Input • P0389 - Crankshaft Position Sensor B Circuit Intermittent • P0400 - Exhaust Gas Recirculation Flow Malfunction • P0401 - Exhaust Gas Recirculation (EGR) Flow Insufficient • P0402 - Exhaust Gas Recirculation Flow Excessive Detected • P0403 - Exhaust Gas Recirculation (EGR) Solenoid Control Circuit • P0404 - Exhaust Gas Recirculation (EGR) Open Position Performance • P0405 - Exhaust Gas Recirculation (EGR) Position Sensor Circuit Low Voltage
    8. • P0406 - Exhaust Gas Recirculation Sensor A Circuit High • P0407 - Exhaust Gas Recirculation Sensor B Circuit Low • P0408 - Exhaust Gas Recirculation Sensor B Circuit High • P0410 - Secondary Air Injection (AIR) System • P0411 - Secondary Air Injection (AIR) System • P0412 - Secondary Air Injection (AIR) Solenoid Relay Control Circuit Bank 1 • P0413 - Secondary Air Injection System Switching Valve A Circuit Open • P0414 - Secondary Air Injection System Switching Valve A Circuit Shorted • P0415 - Secondary Air Injection System Switching Valve B Circuit Malfunction • P0416 - Secondary Air Injection System Switching Valve B Circuit Open • P0417 - Secondary Air Injection System Switching Valve B Circuit Shorted • P0418 - Secondary Air Injection (AIR) Pump Relay Control Circuit Bank 1 • P0419 - Secondary Air Injection (AIR) Pump Relay Control Circuit Bank 2 • P0420 - Catalyst System Low Efficiency • P0421 - Warm Up Catalyst Efficiency Below Threshold (Bank 1) • P0422 - Catalyst System Low Efficiency Bank 1 • P0423 - Heated Catalyst Efficiency Below Threshold (Bank 1) • P0424 - Heated Catalyst Temperature Below Threshold (Bank 1) • P0430 - Catalyst System Low Efficiency Bank 2 • P0431 - Warm Up Catalyst Efficiency Below Threshold (Bank 2) • P0432 - Catalyst System Low Efficiency Bank 2 • P0433 - Heated Catalyst Efficiency Below Threshold (Bank 2) • P0434 - Heated Catalyst Temperature Below Threshold (Bank 2) • P0440 - Evaporative Emission (EVAP) System • P0441 - Evaporative Emission Control System Incorrect Purge Flow • P0442 - Evaporative Emission (EVAP) System Small Leak Detected • P0443 - EVAP Purge Solenoid Valve 1 Control Circuit • P0444 - Evaporative Emission Control System Purge Control Valve Circuit Open • P0445 - Evaporative Emission Control System Purge Control Valve Circuit Shorted • P0446 - EVAP Vent Solenoid Valve Control System • P0447 - Evaporative Emission Control System Vent Control Circuit Open • P0448 - Evaporative Emission Control System Vent Control Circuit Shorted • P0449 - Evaporative Emission (EVAP) Vent Solenoid Control Circuit • P0450 - Fuel Tank Pressure Sensor Circuit • P0451 - Evaporative Emission Control System Pressure Sensor Range/Performance • P0452 - Fuel Tank Pressure Sensor Circuit Low Voltage • P0453 - Fuel Tank Pressure Sensor Circuit High Voltage • P0454 - Evaporative Emission Control System Pressure Sensor Intermittent • P0455 - Evaporative Emission (EVAP) System Leak Detected • P0460 - Fuel Level Sensor Circuit • P0461 - Fuel Level Sensor Performance • P0462 - Fuel Level Sensor Circuit Low Voltage • P0463 - Fuel Level Sensor Circuit High Voltage
    9. • P0464 - Fuel Level Sensor Circuit Intermittent • P0465 - Purge Flow Sensor Circuit Malfunction • P0466 - Purge Flow Sensor Circuit Range/Performance • P0467 - Purge Flow Sensor Circuit Low Input • P0468 - Purge Flow Sensor Circuit High Input • P0469 - Purge Flow Sensor Circuit Intermittent • P0470 - Exhaust Pressure Sensor Malfunction • P0471 - Exhaust Pressure Sensor Range/Performance • P0472 - Exhaust Pressure Sensor Low • P0473 - Exhaust Pressure Sensor High • P0474 - Exhaust Pressure Sensor Intermittent • P0475 - Exhaust Pressure Control Valve Malfunction • P0476 - Exhaust Pressure Control Valve Range/Performance • P0477 - Exhaust Pressure Control Valve Low • P0478 - Exhaust Pressure Control Valve High • P0479 - Exhaust Pressure Control Valve Intermittent • P0480 - Cooling Fan Relay 1 Control Circuit • P0481 - Cooling Fan Relay 2 Control Circuit • P0482 - Cooling Fan 3 Control Circuit Malfunction • P0483 - Cooling Fan Rationality Check Malfunction • P0484 - Cooling Fan Circuit Over Current • P0485 - Cooling Fan Power/Ground Circuit Malfunction • P0496 - Evaporative Emission (EVAP) System Flow During Non-Purge • P0500 - Vehicle Speed Sensor (VSS) Circuit • P0501 - Vehicle Speed Sensor Range/Performance • P0502 - Vehicle Speed Sensor (VSS) Circuit Low Input • P0503 - Vehicle Speed Sensor (VSS) Circuit Intermittent • P0505 - Idle Control System Malfunction • P0506 - Idle Speed Low • P0507 - Idle Speed High • P0510 - Closed Throttle Position Switch Malfunction • P0512 - Start Switch Circuit • P0520 - Engine Oil Pressure Sensor/Switch Circuit Malfunction • P0521 - Engine Oil Pressure Sensor/Switch Circuit Range/Performance • P0522 - Engine Oil Pressure Sensor/Switch Circuit Low Voltage • P0523 - Engine Oil Pressure Sensor/Switch Circuit High Voltage • P0526 - Cooling Fan Speed Sensor Circuit • P0530 - A/C Refrigerant Pressure Sensor Circuit Malfunction • P0531 - A/C Refrigerant Pressure Sensor Circuit Range/Performance • P0532 - Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit Low Voltage • P0533 - Air Conditioning (A/C) Refrigerant Pressure Sensor Circuit High Voltage • P0534 - Air Conditioner Refrigerant Charge Loss • P0550 - Power Steering Pressure (PSP) Switch Circuit • P0551 - Power Steering Pressure Sensor Circuit Range/Performance
    10. • P0552 - Power Steering Pressure Sensor Circuit Low Input • P0553 - Power Steering Pressure Sensor Circuit High Input • P0554 - Power Steering Pressure Sensor Circuit Intermittent • P0560 - System Voltage • P0561 - System Voltage Unstable • P0562 - System Voltage Low (TCM) • P0563 - System Voltage High (TCM) • P0564 - Cruise Control Multi-Function Switch Circuit (PCM) • P0565 - Cruise Control On Signal Malfunction • P0566 - Cruise Control Off Signal Malfunction • P0567 - Cruise Control Resume Signal Malfunction • P0568 - Cruise Control Set Signal Malfunction • P0569 - Cruise Control Coast Signal Malfunction • P0570 - Cruise Control Accel Signal Malfunction • P0571 - Cruise Control Brake Switch Circuit • P0573 - Cruise Control/Brake Switch A Circuit High • P0574 - Vehicle Speed Too High - above 110 mph - Cruise Control Disabled • P0575 - Cruise Control Related Malfunction • P0576 - Cruise Control Related Malfunction • P0576 - Cruise Control Related Malfunction • P0578 - Cruise Control Related Malfunction • P0579 - Cruise Control Related Malfunction • P0580 - Cruise Control Related Malfunction • P0600 - Serial Communication Link Malfunction • P0601 - Control Module Read Only Memory (ROM) • P0602 - Control Module Not Programmed • P0603 - Control Module Long Term Memory Reset • P0604 - Control Module Random Access Memory (RAM) • P0605 - Control Module Programming Read Only Memory (ROM) • P0606 - Control Module Internal Performance • P0607 - ECU Malfunction • P0608 - Control Module VSS Output "A" Malfunction • P0609 - Control Module VSS Output "B" Malfunction • P0610 - Control Module Vehicle Options Incorrect • P0615 - Starter Relay Control Circuit • P0616 - Starter Relay Control Circuit Low Voltage • P0617 - Starter Relay Control Circuit High Voltage • P0620 - Generator Control Circuit Malfunction • P0621 - Generator L-Terminal Circuit • P0622 - Generator F-Terminal Circuit • P0625 - Generator F-Terminal Circuit Low Voltage • P0626 - Generator F-Terminal Circuit High Voltage • P0628 - Fuel Pump Relay Control Circuit Low Voltage • P0629 - Fuel Pump Relay Control Circuit High Voltage • P0638 - Throttle Actuator Control (TAC) Command Performance
    11. • P0641 - PCM voltage out of tolerance condition on the 5-volt reference circuit • P0645 - Air Conditioning (A/C) Clutch Relay Control Circuit • P0646 - Air Conditioning (A/C) Clutch Relay Control Circuit • P0647 - Air Conditioning (A/C) Clutch Relay Control Circuit • P0650 - Malfunction Indicator Lamp (MIL) Control Circuit • P0651 - PCM voltage out of tolerance condition on the 5-volt reference circuit • P0654 - Engine RPM Output Circuit Malfunction • P0655 - Engine Hot Lamp Output Control Circuit Malfucntion • P0656 - Fuel Level Output Circuit Malfunction • P0660 - Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit • P0661 - Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit Low Voltage • P0662 - Intake Manifold Tuning (IMT) Valve Solenoid Control Circuit High Voltage • P0685 - Engine Controls Ignition Relay Control Circuit (PCM) • P0691 - Cooling Fan Relay Control Circuit Low Voltage • P0693 - Cooling Fan Relay Control Circuit Low Voltage • P0692 - Cooling Fan Relay Control Circuit High Voltage • P0694 - Cooling Fan Relay Control Circuit High Voltage • P0700 - Transmission Control System Malfunction • P0701 - Transmission Control System Range/Performance • P0702 - Transmission Control System Electrical • P0703 - Brake Switch Circuit Malfunction • P0704 - Clutch Switch Input Circuit Malfunction • P0705 - Trans Range Switch Circuit • P0706 - Trans Range Switch Performance • P0707 - Transmission Range Sensor Circuit Low Input • P0708 - Transmission Range Sensor Circuit High Input • P0709 - Transmission Range Sensor Circuit Intermittent • P0710 - Transmission Fluid Temperature Sensor Circuit Malfunction • P0711 - TFT Sensor Circuit Range/Performance • P0712 - Transmission Fluid Temperature (TFT) Sensor Circuit Low Input • P0713 - Transmission Fluid Temperature (TFT) Sensor Circuit High Input • P0714 - Transmission Fluid Temperature Sensor Circuit Intermittent • P0715 - Input/Turbine Speed Sensor Circuit Malfunction • P0716 - Input Speed Sensor Circuit Intermittent • P0717 - Input Speed Sensor Circuit Low Input • P0718 - Input/Turbine Speed Sensor Circuit Intermittent • P0719 - Brake Switch Circuit Low Input • P0720 - Output Speed Sensor Circuit Malfunction • P0721 - Output Speed Sensor Range/Performance • P0722 - Output Speed Sensor Circuit Low Input • P0723 - Output Speed Sensor Intermittent • P0724 - Brake Switch Circuit High Input • P0725 - Engine Speed Input Circuit
    12. • P0726 - Engine Speed Input Circuit Range/Performance • P0727 - Engine Speed Circuit No Signal • P0728 - Engine Speed Input Circuit Intermittent • P0730 - Incorrect Gear Ratio • P0731 - Incorrect 1st Gear Ratio • P0732 - Incorrect 2nd Gear Ratio • P0733 - Incorrect 3rd Gear Ratio • P0734 - Incorrect 4th Gear Ratio • P0735 - Gear 5 Incorrect ratio • P0736 - Reverse incorrect gear ratio • P0740 - TCC Enable Solenoid Circuit Electrical • P0741 - TCC System Stuck Off • P0742 - TCC System Stuck On • P0743 - TCC Enable Solenoid Circuit Electrical • P0744 - Torque Converter Clutch Circuit Intermittent • P0745 - Pressure Control Solenoid Malfunction • P0746 - Pressure Control Solenoid Performance or Stuck Off • P0747 - Pressure Control Solenoid Stuck On • P0748 - Pressure Control Solenoid Circuit Electrical • P0749 - Pressure Control Solenoid Intermittent • P0750 - Shift Solenoid A Malfunction • P0751 - 1-2 Shift Solenoid Valve Performance - No First or Fourth Gear • P0752 - 1-2 Shift Solenoid Valve Performance - No Second or Third Gear • P0753 - 1-2 Shift Solenoid Circuit Electrical • P0754 - Shift Solenoid A Intermittent • P0755 - Shift Solenoid B Malfunction • P0756 - 2-3 Shift Solenoid Valve Performance - No First or Second Gear • P0757 - 2-3 Shift Solenoid Valve Performance - No Third or Fourth Gear • P0758 - 2-3 Shift Solenoid Circuit Electrical • P0759 - Shift Solenoid B Intermittent • P0760 - Shift Solenoid C Malfunction • P0761 - Shift Solenoid C Performance or Stuck Off • P0762 - Shift Solenoid C Stuck On • P0763 - Shift Solenoid C Electrical • P0764 - Shift Solenoid C Intermittent • P0765 - Shift Solenoid D Malfunction • P0766 - Shift Solenoid D Performance or Stuck Off • P0767 - Shift Solenoid D Stuck On • P0768 - Shift Solenoid D Electrical • P0769 - Shift Solenoid D Intermittent • P0770 - Shift Solenoid E Malfunction • P0771 - Shift Solenoid E Performance or Stuck Off • P0772 - Shift Solenoid E Stuck On • P0773 - Shift Solenoid E Electrical • P0774 - Shift Solenoid E Intermittent
    13. • P0780 - Shift Malfunction • P0781 - 1-2 Shift Malfunction • P0782 - 2-3 Shift Malfunction • P0783 - 3-4 Shift Malfunction • P0784 - 4-5 Shift Malfunction • P0785 - 3-2 Shift Solenoid Circuit Electrical • P0786 - Shift/Timing Solenoid Range/Performance • P0787 - Shift/Timing Solenoid Low • P0788 - Shift/Timing Solenoid High • P0789 - Shift/Timing Solenoid Intermittent • P0790 - Normal/Performance Switch Circuit Malfunction • P0801 - Reverse Inhibit Control Circuit Malfunction • P0803 - 1-4 Upshift (Skip Shift) Solenoid Control Circuit Malfunction • P0804 - 1-4 Upshift (Skip Shift) Lamp Control Circuit Malfunction • P0850 - Park/Neutral Position (PNP) Switch Circuit • P0856 - Powertrain Indicated Traction Control Malfunction • P0894 - Transmission Component Slipping • P0897 - PCM detects a calculated transmission fluid life of 10 percent or less • P0962 - Line Pressure Control (PC) Solenoid Control Circuit Low Voltage (TCM) • P0963 - Line Pressure Control (PC) Solenoid Control Circuit High Voltage (TCM) • P0966 - Clutch Pressure Control (PC) Solenoid Control Circuit Low Voltage (TCM) • P0967 - Clutch Pressure Control (PC) Solenoid Control Circuit High Voltage (TCM) • P0970 - Shift Pressure control (PC) Solenoid Control Circuit Low Voltage (TCM) • P0971 - Shift Pressure Control (PC) Solenoid Control High Voltage (TCM) • P0973 - PCM detects an open or short to ground in the 1-2 SS valve circuit • P0974 - PCM detects a continuous short to voltage in the 1-2 SS valve circuit • P0976 - PCM detects a continuous open or short to ground in the 2-3 SS valve circuit • P0977 - PCM detects a continuous short to voltage in the 2-3 SS valve circuit • P0979 - Shift Solenoid (SS) 3 Control Circuit Low Voltage (TCM) • P0980 - Shift Solenoid (SS) 3 Control Circuit High Voltage (TCM) • P0982 - Shift Solenoid (SS) 4 Control Circuit High Voltage (TCM) • P0983 - Shift Solenoid (SS) 4 Control Circuit High Voltage (TCM) • P0985 - Shift Solenoid (SS) 5 Control Circuit Low Voltage (TCM) • P0986 - Shift Solenoid (SS) 5 Control Circuit High Voltage (TCM) • P1031 - Heated Oxygen Sensor (HO2S) Heater Current Monitor Control Circuit Banks 1 and 2 Sensor 1 • P1032 - Heated Oxygen Sensor (HO2S) Heater Warm Up Control Circuit Banks 1 and 2 Sensor 1 • P1101 - Actual measured airflow from MAF, MAP, EGR, and TP is not within range of the calculated airflow • P1105 - Secondary Vacuum Sensor Circuit
    14. • P1106 - Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent High Voltage • P1107 - Manifold Absolute Pressure (MAP) Sensor Circuit Intermittent Low Voltage • P1108 - BARO to MAP Sensor Comparison Too High • P1109 - Secondary Port Throttle System • P1111 - Intake Air Temperature (IAT) Sensor Circuit Intermittent High Voltage • P1112 - Intake Air Temperature (IAT) Sensor Circuit Intermittent Low Voltage • P1113 - Intake Resonance Switchover Solenoid Control Circuit • P1114 - Engine Coolant Temperature (ECT) Sensor Circuit Intermittent Low Voltage • P1115 - Engine Coolant Temperature (ECT) Sensor Circuit Intermittent High Voltage • P1116 - ECT Signal Unstable or Intermittent • P1117 - Engine Coolant Temp. Signal Out-Of-Range Low • P1118 - Engine Coolant Temp. Signal Out-Of-Range High • P1119 - ECT Signal Out-Of-Range With TFT Sensor • P1120 - Throttle Position (TP) Sensor 1 Circuit • P1121 - Throttle Position (TP) Sensor Circuit Intermittent High Voltage • P1122 - Throttle Position (TP) Sensor Circuit Intermittent Low Voltage • P1125 - Accelerator Pedal Position (APP) System • P1130 - Heated Oxygen Sensor (HO2S) Circuit Low Variance Bank 1 Sensor 1 • P1131 - Heated Oxygen Sensor (HO2S) Circuit Low Variance Bank 1 Sensor 2 • P1132 - Heated Oxygen Sensor (HO2S) Circuit Low Variance Bank 2 Sensor 1 • P1133 - Heated Oxygen Sensor (HO2S) Insufficient Switching Bank 1 Sensor 1 • P1134 - Heated Oxygen Sensor (HO2S) Transition Time Ratio Bank 1 Sensor 1 • P1135 - Heated Oxygen Sensor (HO2S) Lean Mean Bank 1 Sensor 1 • P1136 - Heated Oxygen Sensor (HO2S) Rich Mean Bank 1 Sensor 1 • P1137 - Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 Lean System or Low Voltage • P1138 - Heated Oxygen Sensor (HO2S) Bank 1 Sensor 2 Rich or High Voltage • P1139 - Heated Oxygen Sensor (HO2S) Insuff. Switching Bank 1 Sensor 2 • P1140 - Heated Oxygen Sensor (HO2S) Transition Time Ratio Bank 1 Sensor 2 • P1141 - Heated Oxygen Sensor (HO2S) Heater Control Circuit Bank 1 Sensor 2 • P1143 - Heated Oxygen Sensor (HO2S) Bank 1 Sensor 3 Lean System or Low Voltage • P1144 - Heated Oxygen Sensor (HO2S) Bank 1 Sensor 3 Rich or High Voltage • P1145 - Heated Oxygen Sensor (HO2S) Cross Counts Bank 1 Sensor 3 • P1153 - Heated Oxygen Sensor (HO2S) Insufficient Switching Bank 2 Sensor 1 • P1154 - Heated Oxygen Sensor (HO2S) Transition Time Ratio Bank 2 Sensor 1 • P1155 - Heated Oxygen Sensor (HO2S) Lean Mean Bank 2 Sensor 1 • P1156 - Heated Oxygen Sensor (HO2S) Rich Mean Bank 2 Sensor 1 • P1157 - Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 Lean System or Low Voltage • P1158 - Heated Oxygen Sensor (HO2S) Bank 2 Sensor 2 Rich or High Voltage
    15. • P1159 - Heated Oxygen Sensor (HO2S) Cross Counts Bank 2 Sensor 2 • P1161 - Heated Oxygen Sensor (HO2S) Heater Control Circuit Bank 2 Sensor 2 • P1163 - Heated Oxygen Sensor (HO2S) Bank 2 Sensor 3 Lean System or Low Voltage • P1164 - Heated Oxygen Sensor (HO2S) Bank 2 Sensor 3 Rich or High Voltage • P1165 - Heated Oxygen Sensor (HO2S) Cross Counts Bank 2 Sensor 3 • P1170 - Bank to Bank Fuel Trim Offset • P1171 - Fuel System Lean During Acceleration • P1172 - Fuel Transfer Pump Flow Insufficient • P1185 - Engine Oil Temperature Circuit • P1186 - EOT Circuit Performance • P1187 - EOT Sensor Circuit Low Voltage • P1188 - EOT Sensor Circuit High Voltage • P1189 - Engine Oil Pressure (EOP) Switch Circuit • P1190 - Engine Vacuum Leak • P1191 - Intake Air Duct Air Leak • P1200 - Injector Control Circuit • P1201 - (Alt. Fuel) Gas Mass Sensor Circuit Range/Performance • P1202 - (Alt. Fuel) Gas Mass Sensor Circuit Low Frequency • P1203 - (Alt. Fuel) Gas Mass Sensor Circuit High Frequency • P1211 - Mass Air Flow Circuit Intermittent High • P1212 - Mass Air Flow Circuit Intermittent Low • P1214 - Injection Pump Timing Offset • P1215 - Ground Fault Detection Indicated • P1216 - Fuel Solenoid Response Time Too Short • P1217 - Fuel Solenoid Response Time Too Long • P1218 - Injection Pump Calibration Circuit • P1219 - Throttle Position Sensor Reference Voltage • P1220 - Throttle Position (TP) Sensor 2 Circuit • P1221 - Fuel Pump Secondary Circuit Low • P1222 - Injector Control Circuit Intermittent • P1225 - Injector Circuit Cylinder 2 Intermittent • P1228 - Injector Circuit Cylinder 3 Intermittent • P1231 - Injector Circuit Cylinder 4 Intermittent • P1234 - Injector Circuit Cylinder 5 Intermittent • P1237 - Injector Circuit Cylinder 6 Intermittent • P1240 - Injector Circuit Cylinder 7 Intermittent • P1243 - Injector Circuit Cylinder 8 Intermittent • P1245 - Intake Plenum Switchover Valve • P1250 - Early Fuel Evaporation Heater Circuit • P1257 - Supercharger System Overboost • P1258 - Engine Coolant Overtemperature - above 268°F - Protection Mode Active • P1260 - Last Test Failed Failed SCC ENTER:More Info. • P1270 - Accelerator Pedal Position Sensor A/D Converter Error
    16. • P1271 - Accelerator Pedal Position (APP) Sensor 1-2 Correlation • P1272 - Accelerator Pedal Position Sensor 2 • P1273 - "Accelerator Pedal Position Sensor 1 • P1274 - Injectors Wired Incorrectly • P1275 - Accelerator Pedal Position (APP) Sensor 1 Circuit • P1276 - Accelerator Pedal Position Sensor 1 Circuit Performance • P1277 - Accelerator Pedal Position Sensor 1 Circuit Low Voltage • P1278 - Accelerator Pedal Position Sensor 1 Circuit High Voltage • P1280 - Accelerator Pedal Position (APP) Sensor 2 Circuit • P1281 - Accelerator Pedal Position Sensor 2 Circuit Performance • P1282 - Accelerator Pedal Position Sensor 2 Circuit Low Voltage • P1283 - Accelerator Pedal Position Sensor 2 Circuit High Voltage • P1285 - Accelerator Pedal Position Sensor 3 Circuit • P1286 - Accelerator Pedal Position Sensor 3 Circuit Performance • P1287 - Accelerator Pedal Position Sensor 3 Circuit Low Voltage • P1288 - Accelerator Pedal Position Sensor 3 Circuit High Voltage • P1300 - Ignitor Circuit • P1305 - Ignition Coil 2 Primary Feedback Circuit • P1310 - Ignition Coil 3 Primary Feedback Circuit • P1315 - Ignition Coil 4 Primary Feedback Circuit • P1320 - IC 4X Reference Circuit Intermittent • P1321 - Electronic Ignition System Fault Line • P1322 - EI System or Ignition Control Extra or Missing • P1323 - IC 24X Reference Circuit Low Frequency • P1324 - Crank RPM Too Low • P1335 - CKP Circuit • P1336 - Crankshaft Position (CKP) System Variation Not Learned • P1345 - Crankshaft Position (CKP)-Camshaft Position (CMP) Correlation • P1346 - Intake Camshaft Position [CMP] Sensor System Performance • P1350 - Ignition Control System • P1351 - Ignition Coil Control Circuit High Voltage • P1352 - IC Output High/Pulse Detected when GND_Cyl. 2 • P1353 - IC Output High/Pulse Detected when GND_Cyl. 3 • P1354 - IC Output High/Pulse Detected when GND_Cyl. 4 • P1355 - IC Output High/Pulse Detected when GND_Cyl. 5 • P1356 - IC Output High/Pulse Detected when GND_Cyl. 6 • P1357 - IC Output High/Pulse Detected when GND_Cyl. 7 • P1358 - IC Output High/Pulse Detected when GND_Cyl. 8 • P1359 - Ignition Coil Group 1 Control Circuit • P1360 - Ignition Coil Group 2 Control Circuit • P1361 - Ignition Coil Control Circuit Low Voltage • P1362 - IC Cylinder 2 Not Toggling After Enable • P1363 - IC Cylinder 3 Not Toggling After Enable • P1364 - IC Cylinder 4 Not Toggling After Enable • P1365 - IC Cylinder 5 Not Toggling After Enable
    17. • P1366 - IC Cylinder 6 Not Toggling After Enable • P1367 - IC Cylinder 7 Not Toggling After Enable • P1368 - IC Cylinder 8 Not Toggling After Enable • P1370 - IC 4X Reference Circuit Too Many Pulses • P1371 - IC 4X Reference Circuit Too Few Pulses • P1372 - Crankshaft Position (CKP) Sensor A-B Correlation • P1374 - 3X Reference Circuit • P1375 - IC 24X Reference Circuit High Voltage • P1376 - Ignition Ground Circuit • P1377 - IC Cam Pulse To 4X Reference Pulse • P1380 - Misfire Detected - Rough Road Data Not Available • P1381 - Misfire Detected - No Communication with Brake Control Module • P1390 - Wheel Speed Sensor 1 - G - Sensor Circuit • P1391 - Wheel Speed Sensor 1 - G - Sensor Circuit Performance • P1392 - Wheel Speed Sensor 1 - G - Sensor Circuit Low Voltage • P1393 - Wheel Speed Sensor 1 - G - Sensor Circuit High Voltage • P1394 - Wheel Speed Sensor 1 - G - Sensor Circuit Intermittent • P1395 - Wheel Speed Sensor 2 - G - Sensor Circuit • P1396 - Wheel Speed Sensor 2 - G - Sensor Circuit Performance • P1397 - Wheel Speed Sensor 2 - G - Sensor Circuit Low Voltage • P1398 - Wheel Speed Sensor 2 - G - Sensor Circuit High Voltage • P1399 - Wheel Speed Sensor 2 - G - Sensor Circuit Intermittent • P1403 - Exhaust Gas Recirculation System Valve 1 • P1404 - Exhaust Gas Recirculation (EGR) Closed Position Performance • P1405 - Exhaust Gas Recirculation System Valve 3 • P1406 - EGR Valve Pintle Position Circuit • P1407 - EGR Air Intrusion in Exhaust Supply to EGR Valve • P1408 - Intake Manifold Pressure Sensor Circuit • P1409 - EGR Vacuum System Leak • P1410 - Fuel Tank Pressure System • P1415 - Secondary Air Injection (AIR) System Bank 1 • P1416 - Secondary Air Injection (AIR) System Bank 2 • P1418 - Secondary Air Injection System Relay A Control Circuit High • P1420 - Intake Air Low Pressure Switch Circuit Low Voltage • P1421 - Intake Air Low Pressure Switch Circuit High Voltage • P1423 - Intake Air High Pressure Switch Circuit High Voltage • P1431 - Fuel Level Sensor 2 Circuit Performance • P1432 - Fuel Level Sensor 2 Circuit Low Voltage • P1433 - Fuel Level Sensor 2 Circuit High Voltage • P1441 - Evaporative Emission (EVAP) System Flow During Non-Purge • P1442 - EVAP Vacuum Sw. High Voltage During Ign. On • P1450 - Barometric Pressure Sensor Circuit • P1451 - Barometric Press. Sensor Performance • P1460 - Cooling Fan Control System • P1480 - Cooling Fan 1 Control Circuit High
    18. • P1481 - Cooling Fan Speed Sensor Circuit • P1482 - Cooling Fan Speed Output Circuit • P1483 - Engine Cooling System Performance • P1484 - Cooling Fan System Performance • P1500 - Starter Signal Circuit • P1501 - Theft Deterrent System • P1501 - Vehicle Speed Sensor Circuit Intermittent • P1502 - Theft Deterrent Fuel Enable Signal Not Received • P1503 - Theft Deterrent Fuel Enable Signal Not Correct • P1504 - Vehicle Speed Output Circuit • P1508 - Idle Speed Low - Idle Air Control (IAC) System Not Responding • P1509 - Idle Speed High - Idle Air Control (IAC) System Not Responding • P1510 - Throttle Control System Performance - Throttle Limitation Active • P1511 - Throttle Control System - Backup System Performance • P1514 - Airflow to TP Sensor Correlation High • P1515 - Electronic Throttle System Throttle Position • P1516 - Throttle Actuator Control (TAC) Module Throttle Actuator Position Performance • P1517 - Electronic Throttle Module • P1518 - Electronic Throttle Module to PCM Communication • P1519 - Throttle Actuator Control (TAC) Module Internal Circuit • P1520 - Transmission Range Switch Circuit • P1521 - Transmission Engaged at High Throttle Angle • P1522 - Park/Neutral to Drive/Reverse at High RPM • P1523 - Throttle Closed Position Performance • P1524 - Throttle Closed Position Performance • P1525 - Throttle Body ServiceRequired • P1526 - Minimum Throttle Position Not Learned • P1527 - Transmission Range to Pressure Switch Correlation • P1528 - Governor • P1529 - Heated Windshield Request Problem • P1530 - Throttle Actuator Control (TAC) Module Internal Circuit • P1531 - A/C Low Side Temperature Sensor Fault • P1532 - A/C Evaporator Temp. Sens. Circuit Low Voltage • P1533 - A/C Evaporator Temp. Sens. Circuit High Voltage • P1534 - A/C High Side Temp. Sensor Low Voltage • P1535 - A/C High Side Temperature Sensor Circuit • P1536 - Engine Coolant Overtemperature - Air Conditioning (A/C) Disabled • P1537 - A/C Request Circuit Low Voltage • P1538 - A/C Request Circuit High Voltage • P1539 - A/C Clutch Status Circuit High Voltage • P1540 - Air Conditioning (A/C) Refrigerant Overpressure - Air Conditioning (A/C) Disabled • P1541 - A/C High Side Over Temperature • P1542 - A/C System High Pressure High Temperature
    19. • P1543 - A/C System Performance • P1544 - A/C Refrigerant Condition Very Low • P1545 - Air Conditioning (A/C) Clutch Relay Control Circuit • P1546 - A/C Clutch Status Circuit Low Voltage • P1547 - A/C System Performance Degraded • P1548 - A/C Recirculation Circuit • P1551 - Throttle Valve Rest Position Not Reached During Learn • P1554 - Cruise Control Feedback Circuit • P1555 - Electronic Variable Orifice Output • P1558 - Cruise Control Servo Indicates Low • P1559 - Cruise Control Power Management Mode • P1560 - Transaxle Not in Drive - Cruise Control Disabled • P1561 - Cruise Vent Solenoid • P1562 - Cruise Vacuum Solenoid • P1563 - Cruise Vehicle Speed/Set Speed Difference Too High • P1564 - Vehicle Acceleration Too High - Cruise Control Disabled • P1565 - Cruise Servo Position Sensor • P1566 - Engine RPM Too High - Cruise Control Disabled • P1567 - Active Banking Control Active - Cruise Control Disabled • P1568 - Cruise Servo Stroke Greater than Commanded in Cruise • P1569 - Cruise Servo Stroke High While not in Cruise • P1570 - Traction Control Active - Cruise Control Disabled • P1571 - Traction Control Torque Request Circuit • P1572 - ASR Active Circuit Low Too Long • P1573 - PCM/EBTCM Serial Data Circuit • P1574 - Stoplamp Switch Circuit • P1575 - Extended Travel Brake Switch Circuit • P1576 - BBV Sensor Circuit High Voltage • P1577 - BBV Sensor Circuit Low Voltage • P1578 - BBV Sensor Circuit Low Vacuum • P1579 - P/N to D/R at High Throttle Angle - Power Reduction Mode Active • P1580 - Cruise Move Circuit Low Voltage • P1581 - Cruise Move Circuit High Voltage • P1582 - Cruise Direction Circuit Low Voltage • P1583 - Cruise Direction CircuitHigh Voltage • P1584 - Cruise Control Disabled • P1585 - Cruise Control Inhibit Output Circuit • P1586 - Cruise Control Brake Switch 2 Circuit • P1587 - Cruise Control Clutch Control Circuit Low • P1588 - Cruise Control Clutch Control Circuit High • P1599 - Engine Stall or Near Stall Detected • P1600 - TCM Internal Watchdog Operation • P1601 - Serial Comm. Problem With Device 1 • P1602 - Knock Sensor (KS) Module Performance • P1603 - Loss of SDM Serial Data
    20. • P1604 - Loss of IPC Serial Data • P1605 - Loss of HVAC Serial Data • P1606 - Serial Communication Problem With Device 6 • P1607 - Serial Communication Problem With Device 7 • P1608 - Serial Communication Problem With Device 8 • P1609 - Loss Of TCS Serial Data • P1610 - Loss of PZM Serial Data • P1611 - Loss of CVRTD Serial Data • P1612 - Loss of IPM Serial Data • P1613 - Loss of DIM Serial Data • P1614 - Loss of RIM Serial Data • P1615 - Loss of VTD Serial Data • P1617 - Engine Oil Level Switch Circuit • P1619 - Engine Oil Life Monitor Reset Circuit • P1620 - Low Coolant Circuit • P1621 - Control Module Long Term Memory Performance • P1622 - Cylinder Select • P1623 - Transmission Temp Pull-Up Resistor • P1624 - Customer Snapshot Requested - Data Available • P1625 - TCM System Reset • P1626 - Theft Deterrent Fuel Enable Signal Not Received • P1627 - A/D Performance • P1628 - ECT Pull-Up Resistor • P1629 - Theft Deterrent System - Cranking Signal • P1630 - Theft Deterrent Learn Mode Active • P1631 - Theft Deterrent Start Enable Signal Not Correct • P1632 - Theft Deterrent Fuel Disable Signal Received • P1633 - Ignition 0 Switch Circuit • P1634 - Ignition 1 Switch Circuit • P1635 - 5 Volt Reference Circuit • P1636 - PCM Stack Overrun • P1637 - Generator L-Terminal Circuit • P1638 - Generator F-Terminal Circuit • P1639 - 5 Volt Reference 2 Circuit • P1640 - Driver-1-Input High Voltage • P1641 - Malfunction Indicator Lamp (MIL) Control Circuit • P1642 - Vehicle Speed Output Circuit • P1643 - Engine Speed Output Circuit • P1644 - Traction Control Delivered Torque Output Circuit • P1645 - Evaporative Emission (EVAP) Vent Solenoid Contorl Circuit • P1646 - Evaporative Emission (EVAP) Vent Solenoid Control Circuit • P1647 - Driver 1 Line 7 • P1650 - Control Module Output B Circuit • P1651 - Fan 1 Relay Control Circuit • P1652 - Powertrain Induced Chassis Pitch Output Circuit
    21. • P1653 - Oil Level Lamp Control Circuit • P1654 - Cruise Control Inhibit Output Circuit • P1655 - EVAP Purge Solenoid Control Circuit • P1656 - Driver 2 Line 6 • P1657 - 1-4 Upshift Solenoid Control Circuit • P1658 - Starter Enable Relay Control Circuit • P1660 - Cooling Fan Control Circuits • P1661 - MIL Control Circuit • P1662 - Cruise Lamp Control Circuit • P1663 - Oil Life Lamp Control Circuit • P1664 - 1-4 Upshift Lamp Control Circuit • P1665 - Driver 3 Line 5 • P1666 - Driver 3 Line 6 • P1667 - Reverse Inhibit Solenoid Control Circuit • P1669 - ABS Unit Expected • P1670 - Driver 4 • P1671 - Driver 4 Line 1 • P1672 - Low Engine Oil Level Lamp Control Circuit • P1673 - Engine Hot Lamp Control Circuit • P1674 - Tachometer Control Circuit • P1675 - EVAP Vent Solenoid Control Circuit • P1676 - Driver 4 Line 6 • P1677 - Driver 4 Line 7 • P1680 - Driver 5 (ECU Malfunction) • P1681 - Driver 5 Line 1 • P1682 - Driver 5 Line 2 • P1683 - Driver 5 Line 3 • P1684 - Driver 5 Line 4 • P1685 - Driver 5 Line 5 • P1686 - Driver 5 Line 6 • P1687 - Driver 5 Line 7 • P1689 - Delivered Torque Circuit Fault • P1690 - ECM Loop Overrun • P1691 - Coolant Gage Circuit Low Voltage • P1692 - Coolant Gage Circuit High Voltage • P1693 - Tachometer Circuit Low Voltage • P1694 - Tachometer Circuit High Voltage • P1695 - Remote Keyless Entry Circuit Low • P1696 - Remote Keyless Entry Voltage High • P1700 - Transmission Control Module (TCM) Requested MIL Illumination • P1701 - Trans. MIL Request Circuit • P1705 - P/N Signal Output Circuit • P1719 - Incorrect Shifting Detected (TCM) • P1740 - Torque Reduction Signal Circuit • P1743 - TP Signal from ECM
    22. • P1760 - TCM Supply Voltage Interrupted • P1779 - Engine Torque Delivered to TCM Signal • P1780 - Park/Neutral Position [PNP] Switch Circuit • P1781 - Engine Torque Signal Circuit • P1790 - Transmission Control Module Checksum • P1791 - Transmission Control Module Loop • P1791 - Throttle/Pedal Position Signal (2000+) • P1792 - Transmission Control Module Reprogrammable Memory • P1792 - ECM to TCM Engine Coolant Signal • P1793 - Transmission Control Module Stack Overrun • P1793 - Wheel Speed Signal (2000+) • P1795 - CAN Bus - Throttle Body Position • P1800 - TCM Power Relay Control Circuit • P1801 - Performance Selector Switch Failure • P1804 - Ground Control Relay • P1810 - TFP Valve Position Switch Circuit • P1811 - Maximum Adapt and Long Shift • P1812 - Transmission Over Temperature Condition • P1813 - Torque Control • P1814 - Torque Converter Overstressed • P1815 - Transmission Range Switch - Start In Wrong Range • P1816 - TFP Valve Position Sw. - Park/Neu. With Drive Ratio • P1817 - TFP Valve Position Sw. - Reverse With Drive Ratio • P1818 - TFP Valve Position Sw. - Drive Without Drive Ratio • P1819 - Internal Mode Switch - No StartWrong Range • P1820 - Internal Mode Switch Circuit A Low • P1822 - Internal Mode Switch Circuit B High • P1823 - Internal Mode Switch Circuit P Low • P1825 - Internal Mode Switch - Invalid Range • P1826 - Internal Mode Switch Circuit C - High • P1831 - Pressure Control (PC) Solenoid Power Circuit - Low Voltage • P1832 - Pressure Control (PC)/Shift Lock Solenoid Control Circuit High Voltage • P1833 - A/T Solenoids Power Circuit - Low Voltage • P1834 - Torque Converter Clutch (TCC)/Shift Solenoid (SS) Control Circuit High Voltage • P1835 - Kick-Down Switch Circuit • P1836 - Kick-Down Switch Failed Open • P1837 - Kick-Down Switch Failed Short • P1842 - 1-2 Shift Solenoid Circuit Low Voltage • P1843 - 1-2 Shift Solenoid Circuit High Voltage • P1844 - Torque Reduction Signal Circuit Desired By TCM • P1845 - 2-3 Shift Solenoid Circuit Low Voltage • P1847 - 2-3 Shift Solenoid Circuit High Voltage • P1850 - Brake Band Apply Solenoid Circuit • P1851 - Brake Band Apply Solenoid Performance
    23. • P1852 - Brake Band Apply SolenoidLow Voltage • P1853 - Brake Band Apply Solenoid High Voltage • P1860 - TCC PWM Solenoid Circuit Electrical • P1864 - Torque Converter Clutch Circuit • P1865 - 4-5 Shift Solenoid (SS) Valve Control Circuit High Voltage • P1866 - Torque Converter Clutch (TCC) Pulse Width Modulation (PWM) Solenoid Control Circuit Low Voltage • P1867 - Torque Converter Clutch (TCC) Pulse Width Modulation (PWM) Solenoid Control Circuit High Voltage • P1868 - Transmission Fluid Life • P1870 - Transmission Component Slipping • P1871 - Undefined Gear Ratio • P1873 - TCC Stator Temp. Switch Circuit Low • P1874 - TCC Stator Temp. Switch Circuit High • P1875 - 4WD Low Switch Circuit Electrical • P1884 - TCC Enable/Shift Light Circuit • P1886 - Shift Timing Solenoid • P1887 - TCC Release Switch Circuit • P1890 - ECM Data Input Circuit • P1890 - Throttle Position Signal Input • P1891 - Throttle Position Sensor PWM Signal Low • P1892 - Throttle Position Sensor PWM Signal High • P1893 - Engine Torque Signal Low Voltage • P1894 - Engine Torque Signal High Voltage • P1895 - TCM to ECM Torque Reduction Circuit • P2008 - Intake Manifold Runner Control (IMRC) Solenoid Control Circuit • P2009 - Intake Manifold Runner Control (IMRC) Solenoid Control Circuit Low Voltage • P2010 - Intake Manifold Runner Control (IMRC) Solenoid Control Circuit High Voltage • P2066 - Fuel Level Sensor 2 Performance • P2067 - Fuel Level Sensor 2 Circuit Low Voltage • P2068 - Fuel Level Sensor 2 Circuit High Voltage • P2096 - Post Catalyst Fuel Trim System Low Limit • P2097 - Post Catalyst Fuel Trim System High Limit • P2098 - Post Catalyst Fuel Trim System Low Limit • P2099 - Post Catalyst Fuel Trim System High Limit • P2100 - Throttle Actuator Control (TAC) Motor Control Circuit • P2101 - Control Module Throttle Actuator Position Performance • P2105 - Throttle Actuator Control (TAC) System - Forced Engine Shutdown • P2107 - Throttle Actuator Control (TAC) Module Internal Circuit • P2108 - Throttle Actuator Control (TAC) Module Performance • P2119 - Throttle Closed Position Performance • P2120 - Accelerator Pedal Position (APP) Sensor 1 Circuit • P2121 - Accelerator Pedal Position (APP) Sensor 1 Performance
    24. • P2122 - Accelerator Pedal Position (APP) Sensor 1 Circuit Low Voltage • P2123 - Accelerator Pedal Position (APP) Sensor 1 Circuit High Voltage • P2125 - Accelerator Pedal Position (APP) Sensor 2 Circuit • P2127 - Accelerator Pedal Position (APP) Sensor 2 Circuit Low Voltage • P2128 - Accelerator Pedal Position (APP) Sensor 2 Circuit High Voltage • P2135 - Throttle Position (TP) Sensor 1-2 Correlation • P2138 - Accelerator Pedal Position (APP) Sensor 1-2 Correlation • P2176 - Minimum Throttle Position Not Learned • P2500 - Generator L-Terminal Circuit Low Voltage • P2501 - Generator L-Terminal Circuit High Voltage • P2535 - Ignition 1 Switch Circuit High Voltage (PCM) • P2610 - ECU Malfunction • P2763 - Short to voltage in the TCC Solenoid • P2764 - Open or Short to ground in the TCC PWM solenoid valve circuit • P2A00 - HO2S Circuit Closed Loop (CL) Performance Bank 1 Sensor 1 (PCM) • P2A01 - HO2S Circuit Closed Loop (CL) Performance Bank 1 Sensor 2 (PCM) • P3000 - Hacking AWH Data

