 P1100 - Manifold absolute pressure (MAP) sensor – EGR – circuit malfunction P1102 - Manifold absolute pressure (MAP) sensor – EGR mode 3 P1103 - Manifold absolute pressure (MAP) sensor – EGR mode 2 P1106 - Manifold absolute pressure (MAP) sensor – signal high P1107 - Manifold absolute pressure (MAP) sensor – signal low P1110 - Electronic throttle system (ETS) – malfunction P1111 - Intake air temperature (IAT) sensor- circuit low input/intermittent P1112 - Intake air temperature (IAT) sensor- circuit high input/intermittent P1114 - Engine coolant temperature (ECT) sensor – signal malfunction P1115 - Engine coolant temperature (ECT) sensor – signal malfunction P1118 - Throttle motor – malfunction P1123 - Long term fuel trim – additive – mixture too rich P1124 - Long term fuel trim -additive – mixture too lean P1127 - Long term fuel trim – system too rich P1128 - Long term fuel trim – system too lean P1134 - Heated oxygen sensor (H02S) 1, bank 1 – slow response P1140 - Engine load monitoring (MAFfrP) -signals not plausible P1147 - Accelerator pedal position (APP) sensor 1 – circuit malfunction P1151 - Accelerator pedal position (APP) sensor 2 – circuit malfunction P1152 - Accelerator pedal position (APP) sensor 2 – low voltage P1153 - Accelerator pedal position (APP) sensor 2 – high voltage P1154 - Heated oxygen sensor (H02S) 1, bank 2 – slow response P1155 - Electronic throttle system (ETS) – malfunction P1159 - Intake manifold air control, target position – malfunction P1166 - Heated oxygen sensor (H02S) 1, bank 1 – control limit reached P1167 - Heated oxygen sensor (H02S) 1, bank 2- control limit reached P1168 - Heated oxygen sensor (H02S) 2, bank 1, heater control – circuit malfunction P1169 - Heated oxygen sensor (H02S) 2, bank 2, heater control – circuit malfunction P1171 - Electronic throttle system (ETS), WOT – malfunction P1172 - ETS throttle motor – abnormal current P1173 - ETS throttle motor – abnormal voltage P1174 - Electronic throttle system (ETS), closed throttle 1 – malfunction
2. P1175 - Electronic throttle system (ETS), closed throttle 2 – malfunction P1176 - ETS throttle motor – circuit 1 malfunction P1177 ETS throttle motor – circuit 2 malfunction P1178 - Electronic throttle system (ETS) relay – malfunction P1184 - Heated oxygen sensor (H02S) 1, bank 2 – no activity detected P1191 - Electronic throttle system (ETS), limp-home valve – malfunction P1192 - Electronic throttle system (ETS) – limp-home valve ON P1193 - Electronic throttle system (ETS) – limp-home valve ON P1194 - Electronic throttle system (ETS) – limp-home valve ON P1195 - Electronic throttle system (ETS) – limp-home valve ON P1196 - Electronic throttle system (ETS) – limp-home valve ON P1295 - Electronic throttle system (ETS) – circuit malfunction P1307 - Rough road sensor – malfunction P1308 - Rough road sensor – voltage low P1309 - Rough road sensor – voltage high P1330 - Ignition spark timing – malfunction P1372 - Vehicle speed sensor (VSS) – range/performance problem P1400 - Exhaust gas recirculation (EGR) system – monitor malfunction P1401 - Fuel tank leakage diagnostic module -system malfunction P1402 - Fuel tank leakage diagnostic module – motor malfunction P1403 - Fuel tank leakage diagnostic module – valve malfunction P1404 - Fuel tank leakage diagnostic module – heater malfunction P1440 - Evaporative emission (EVAP) system, vent valve – circuit malfunction P1502 - Wheel speed sensor – open circuit P1503 - Cruise control switch – circuit malfunction P1504 - Cruise control switch, CANCEL – circuit malfunction P1505 - Idle air control (lAC) valve – opening coil circuit – open circuit P1506 - Idle air control (lAC) valve – opening coil circuit – short circuit P1507 - Idle air control (lAC) valve – closing coil circuit – open circuit P1508 - Idle air control (lAC) valve – closing coil circuit – short circuit P1510 - Idle air control (lAC) valve – circuit malfunction – open/short circuit P1511 - Idle air control {lAC) valve – circuit malfunction – open/short circuit P1513 - Idle air control (lAC) valve – opening coil circuit – short circuit P1515 - Idle air control (lAC) valve – coil 1 – signal malfunction
3. P1516 - Idle air control {lAC) valve – coil 2 – signal malfunction P1520 - Alternator – FR terminal malfunction P1521 - Power steering pressure (PSP) switch – circuit malfunction P1523 - Intake manifold air control solenoid P1529 - Transmission control module (TCM) – communication P1550 - Knock sensor (KS) – signal malfunction P1552 - Idle air control (lAC) valve – closing coil circuit – short circuit P1553 - Idle air control (lAC) valve – closing coil circuit – open circuit P1560 - Knock sensor (KS) – signal malfunction P1586 - AT coding – signal not plausible P1602 - Transmission control module (TCM) – serial communication problem P1605 - G-force sensor – circuit malfunction P1606 - G-force sensor – signal not plausible P1607 - Engine control module (ECM)/electronic throttle system (ETS) – communication malfunction P1608 - Electronic throttle system (ETS)/engine control module (ECM) – communication malfunction P1609 - Immobilizer control module – malfunction P1611 - MIL request signal – circuiVvoltage low P1613-D - MIL request signal – circuiVvoltage high P1613-9 - Electronic throttle system (ETS), controller- malfunction P1614-B - MIL request signal – circuiVvoltage high P1614-9 - Electronic throttle system (ETS), EEPROM RJW – malfunction P1615 - Electronic throttle system (ETS), controller- malfunction P1616 - Engine control relay – circuit malfunction P1618 - Engine torque control – limit reached/exceeded P1623 - Malfunction indicator lamp (MIL) – circuit malfunction P1624 - Engine coolant blower motor relay -low speed circuit malfunction P1625 - Engine coolant blower motor relay – high speed circuit malfunction P1632 - CAN data bus OFF P1632 - Traction control system – malfunction P1642 - Engine control module (ECM) – non immobilizer/incorrect type P1665 - Ignition power stage A – circuit malfunction P1670 - Ignition power stage B – circuit malfunction P1690 - Immobilizer system – malfunction
4. P1691 - Immobilizer system – antenna malfunction P1693-0 - Transmission control module (TCM) MIL request circuit – circuit malfunction P1693-fJ - Immobilizer system – transponder malfunction P1694 - Immobilizer system – ECM signal malfunction P1695 - Immobilizer system – ECM EPROM malfunction P1696 - Immobilizer system – ECM EPROM malfunction P1707 - Cruise control, brake pedal position (BPP) switch – circuit malfunction P1715 - AT pulse generators – open circuit P1750 - AT – shift control solenoids P1765 - Transmission control module (TCM) – torque reduction malfunction 
