P1101 - O2 Sensor Circ.,Bank1-Sensor1Voltage too Low/Air Leak P1102 - O2 Sensor Heating Circ.,Bank1-Sensor1 Short to B+ P1103 - O2 Sensor Heating Circ.,Bank1-Sensor1 Output too Low P1104 - Bank1-Sensor2 Voltage too Low/Air Leak P1105 - O2 Sensor Heating Circ.,Bank1-Sensor2 Short to B+ P1106 - O2 Sensor Circ.,Bank2-Sensor1 Voltage too Low/Air Leak P1107 - O2 Sensor Heating Circ.,Bank2-Sensor1 Short to B+ P1108 - O2 Sensor Heating Circ.,Bank2-Sensor1 Output too Low P1109 - O2 Sensor Circ.,Bank2-Sensor2 Voltage too Low/Air Leak P1110 - O2 Sensor Heating Circ.,Bank2-Sensor2 Short to B+ P1111 - O2 Control (Bank 1) System too lean P1112 - O2 Control (Bank 1) System too rich P1113 - Bank1-Sensor1 Internal Resistance too High P1114 - Bank1-Sensor2 Internal Resistant too High P1115 - O2 Sensor Heater Circ.,Bank1-Sensor1 Short to Ground P1116 - O2 Sensor Heater Circ.,Bank1-Sensor1 Open P1117 - O2 Sensor Heater Circ.,Bank1-Sensor2 Short to Ground P1118 - O2 Sensor Heater Circ.,Bank1-Sensor2 Open P1119 - O2 Sensor Heater Circ.,Bank2-Sensor1 Short to Ground P1120 - O2 Sensor Heater Circ.,Bank2-Sensor1 Open P1121 - O2 Sensor Heater Circ.,Bank2-Sensor2 Short to Ground P1122 - O2 Sensor Heater Circ.,Bank2-Sensor2 Open P1123 - Long Term Fuel Trim Add.Air.,Bank1 System too Rich P1124 - Long Term Fuel Trim Add.Air.,Bank1 System too Lean P1125 - Long Term Fuel Trim Add.Air.,Bank2 System too Rich P1126 - Long Term Fuel Trim Add.Air.,Bank2 System too Lean P1127 - Long Term Fuel Trim mult.,Bank1 System too Rich P1128 - Long Term Fuel Trim mult.,Bank1 System too Lean P1129 - Long Term Fuel Trim mult.,Bank2 System too Rich P1130 - Long Term Fuel Trim mult.,Bank2 System too Lean P1131 - Bank2-Sensor1 Internal Rsistance too High P1132 - O2 Sensor Heating Circ.,Bank1+2-Sensor1 Short to B+ P1133 - O2 Sensor Heating Circ.,Bank1+2-Sensor1 Electrical Malfunction
2. P1134 - O2 Sensor Heating Circ.,Bank1+2-Sensor2 Short to B+ P1135 - O2 Sensor Heating Circ.,Bank1+2-Sensor2 Electrical Malfunction P1136 - Long Term Fuel Trim Add.Fuel,Bank1 System too Lean P1137 - Long Term Fuel Trim Add.Fuel,Bank1 System too Rich P1138 - Long Term Fuel Trim Add.Fuel,Bank2 System too Lean P1139 - Long Term Fuel Trim Add.Fuel,Bank2 System too Rich P1140 - Bank2-Sensor2 Internal Resistance too High P1141 - Load Calculation Cross Check Range/Performance P1142 - Load Calculation Cross Check Lower Limit Exceeded P1143 - Load Calculation Cross Check Upper Limit Exceeded P1144 - Mass or Volume Air Flow Circ Open/Short to Ground P1145 - Mass or Volume Air Flow Circ Short to B+ P1146 - Mass or Volume Air Flow Circ Supply Malfunction P1147 - O2 Control (Bank 2) System too lean P1148 - O2 Control (Bank 2) System too rich P1149 - O2 Control (Bank 1) Out of range P1150 - O2 Control (Bank 2) Out of range P1151 - Bank1, Long Term Fuel Trim, Range 1 Leanness Lower Limit Exceeded P1152 - Bank1, Long Term Fuel Trim, Range 2 Leanness Lower Limit Exceeded P1154 - Manifold Switch Over Malfunction P1155 - Manifold Abs.Pressure Sensor Circ. Short to B+ P1156 - Manifold Abs.Pressure Sensor Circ. Open/Short to Ground P1157 - Manifold Abs.Pressure Sensor Circ. Power Supply Malfunction P1158 - Manifold Abs.Pressure Sensor Circ. Range/Performance P1160 - Manifold Temp.Sensor Circ. Short to Ground P1161 - Manifold Temp.Sensor Circ. Open/Short to B+ P1162 - Fuel Temp.Sensor Circ. Short to Ground P1163 - Fuel Temp.Sensor Circ. Open/Short to B+ P1164 - Fuel Temperature Sensor Range/Performance/Incorrect Signal P1165 - Bank1, Long Term Fuel Trim, Range 1 Rich Limit Exceeded P1166 - Bank1, Long Term Fuel Trim, Range 2 Rich Limit Exceeded P1171 - Throttle Actuation Potentiometer Sign.2 Range/Performance P1172 - Throttle Actuation Potentiometer Sign.2 Signal too Low P1173 - Throttle Actuation Potentiometer Sign.2 Signal too High
3. P1174 - Fuel Trim, Bank 1 Different injection times P1176 - O2 Correction Behind Catalyst,B1 Limit Attained P1177 - O2 Correction Behind Catalyst,B2 Limit Attained P1178 - Linear 02 Sensor / Pump Current Open Circuit P1179 - Linear 02 Sensor / Pump Current Short to ground P1180 - Linear 02 Sensor / Pump Current Short to B+ P1181 - Linear 02 Sensor / Reference Voltage Open Circuit P1182 - Linear 02 Sensor / Reference Voltage Short to ground P1183 - Linear 02 Sensor / Reference Voltage Short to B+ P1184 - Linear 02 Sensor / Common Ground Wire Open Circuit P1185 - Linear 02 Sensor / Common Ground Wire Short to ground P1186 - Linear 02 Sensor / Common Ground Wire Short to B+ P1187 - Linear 02 Sensor / Compens. Resistor Open Circuit P1188 - Linear 02 Sensor / Compens. Resistor Short to ground P1189 - Linear 02 Sensor / Compens. Resistor Short to B+ P1190 - Linear 02 Sensor / Reference Voltage Incorrect Signal P1196 - O2 Sensor Heater Circ.,Bank1-Sensor1 Electrical Malfunction P1197 - O2 Sensor Heater Circ.,Bank2-Sensor1 Electrical Malfunction P1198 - O2 Sensor Heater Circ.,Bank1-Sensor2 Electrical Malfunction P1199 - O2 Sensor Heater Circ.,Bank2-Sensor2 Electrical Malfunction P1201 - Cyl.1-Fuel Inj.Circ. Electrical Malfunction P1202 - Cyl.2-Fuel Inj.Circ. Electrical Malfunction P1203 - Cyl.3-Fuel Inj.Circ. Electrical Malfunction P1204 - Cyl.4-Fuel Inj.Circ. Electrical Malfunction P1205 - Cyl.5-Fuel Inj.Circ. Electrical Malfunction P1206 - Cyl.6-Fuel Inj.Circ. Electrical Malfunction P1207 - Cyl.7-Fuel Inj.Circ. Electrical Malfunction P1208 - Cyl.8-Fuel Inj.Circ. Electrical Malfunction P1209 - Intake valves for cylinder shut-off Short circuit to ground P1210 - Intake valves for cylinder shut-off Short to B+ P1211 - Intake valves for cylinder shut-off Open circuit P1213 - Cyl.1-Fuel Inj.Circ. Short to B+ P1214 - Cyl.2-Fuel Inj.Circ. Short to B+ P1215 - Cyl.3-Fuel Inj.Circ. Short to B+
4. P1216 - Cyl.4-Fuel Inj.Circ. Short to B+ P1217 - Cyl.5-Fuel Inj.Circ. Short to B+ P1218 - Cyl.6-Fuel Inj.Circ. Short to B+ P1219 - Cyl.7-Fuel Inj.Circ. Short to B+ P1220 - Cyl.8-Fuel Inj.Circ. Short to B+ P1221 - Cylinder shut-off exhaust valves Short circuit to ground P1222 - Cylinder shut-off exhaust valves Short to B+ P1223 - Cylinder shut-off exhaust valves Open circuit P1225 - Cyl.1-Fuel Inj.Circ. Short to Ground P1226 - Cyl.2-Fuel Inj.Circ. Short to Ground P1227 - Cyl.3-Fuel Inj.Circ. Short to Ground P1228 - Cyl.4-Fuel Inj.Circ. Short to Ground P1229 - Cyl.5-Fuel Inj.Circ. Short to Ground P1230 - Cyl.6-Fuel Inj.Circ. Short to Ground P1231 - Cyl.7-Fuel Inj.Circ. Short to Ground P1232 - Cyl.8-Fuel Inj.Circ. Short to Ground P1237 - Cyl.1-Fuel Inj.Circ. Open Circ. P1238 - Cyl.2-Fuel Inj.Circ. Open Circ. P1239 - Cyl.3-Fuel Inj.Circ. Open Circ. P1240 - Cyl.4-Fuel Inj.Circ. Open Circ. P1241 - Cyl.5-Fuel Inj.Circ. Open Circ. P1242 - Cyl.6-Fuel Inj.Circ. Open Circ. P1243 - Cyl.7-Fuel Inj.Circ. Open Circ. P1244 - Cyl.8-Fuel Inj.Circ. Open Circ. P1245 - Needle Lift Sensor Circ. Short to Ground P1246 - Needle Lift Sensor Circ. Range/Performance P1247 - Needle Lift Sensor Circ. Open/Short to B+ P1248 - Injection Start Control Deviation P1249 - Fuel consumption signal Electrical Fault in Circuit P1250 - Fuel Level Too Low P1251 - Start of Injection Solenoid Circ Short to B+ P1252 - Start of Injection Solenoid Circ Open/Short to Ground P1253 - Fuel consumption signal Short to ground P1254 - Fuel consumption signal Short to B+
5. P1255 - Engine Coolant Temp.Circ Short to Ground P1256 - Engine Coolant Temp.Circ Open/Short to B+ P1257 - Engine Coolant System Valve Open P1258 - Engine Coolant System Valve Short to B+ P1259 - Engine Coolant System Valve Short to Ground P1280 - Fuel Inj.Air Contr.Valve Circ. Flow too Low P1283 - Fuel Inj.Air Contr.Valve Circ. Electrical Malfunction P1284 - Fuel Inj.Air Contr.Valve Circ. Open P1285 - Fuel Inj.Air Contr.Valve Circ. Short to Ground P1286 - Fuel Inj.Air Contr.Valve Circ. Short to B+ P1287 - Turbocharger bypass valve open P1288 - Turbocharger bypass valve short to B+ P1289 - Turbocharger bypass valve short to ground P1296 - Cooling system malfunction P1297 - Connection turbocharger - throttle valve pressure hose P1300 - Misfire detected Reason: Fuel level too low P1319 - Knock Sensor 1 Circ. Short to Ground P1320 - Knock Sensor 2 Circ. Short to Ground P1321 - Knock Sensor 3 Circ. Low Input P1322 - Knock Sensor 3 Circ. High Input P1323 - Knock Sensor 4 Circ. Low Input P1324 - Knock Sensor 4 Circ. High Input P1325 - Cyl.1-Knock Contr. Limit Attained P1326 - Cyl.2-Knock Contr. Limit Attained P1327 - Cyl.3-Knock Contr. Limit Attained P1328 - Cyl.4-Knock Contr. Limit Attained P1329 - Cyl.5-Knock Contr. Limit Attained P1330 - Cyl.6-Knock Contr. Limit Attained P1331 - Cyl.7-Knock Contr. Limit Attained P1332 - Cyl.8-Knock Contr. Limit Attained P1335 - Engine Torque Monitoring 2 Control Limint Exceeded P1336 - Engine Torque Monitoring Adaptation at limit P1337 - Camshaft Pos.Sensor,Bank1 Short to Ground P1338 - Camshaft Pos.Sensor,Bank1 Open Circ./Short to B+
6. P1339 - Crankshaft Pos./Engine Speed Sensor Cross Connected P1340 - Crankshaft-/Camshaft Pos.Sens.Signals Out of Sequence P1341 - Ignition Coil Power Output Stage 1 Short to Ground P1342 - Ignition Coil Power Output Stage 1 Short to B+ P1343 - Ignition Coil Power Output Stage 2 Short to Ground P1344 - Ignition Coil Power Output Stage 2 Short to B+ P1345 - Ignition Coil Power Output Stage 3 Short to Ground P1346 - Ignition Coil Power Output Stage 3 Short to B+ P1347 - Bank2,Crankshaft-/Camshaft os.Sens.Sign. Out of Sequence P1348 - Ignition Coil Power Output Stage 1 Open Circuit P1349 - Ignition Coil Power Output Stage 2 Open Circuit P1350 - Ignition Coil Power Output Stage 3 Open Circuit P1354 - Modulation Piston Displ.Sensor Circ. Malfunction P1355 - Cyl. 1, ignition circuit Open Circuit P1356 - Cyl. 1, ignition circuit Short to B+ P1357 - Cyl. 1, ignition circuit Short to ground P1358 - Cyl. 2, ignition circuit Open Circuit P1359 - Cyl. 2, ignition circuit Short Circuit to B+ P1360 - Cyl. 2, ignition circuit Short Circuit to Ground P1361 - Cyl. 3, ignition circuit Open Circuit P1362 - Cyl. 3, ignition circuit Short Circuit to B+ P1363 - Cyl. 3, ignition circuit Short Circuit to ground P1364 - Cyl. 4 ignition circuit Open Circuit P1365 - Cyl. 4 ignition circuit Short circuit to B+ P1366 - Cyl. 4 ignition circuit Short circuit to ground P1367 - Cyl. 5, ignition circuit Open Circuit P1368 - Cyl. 5, ignition circuit Short Circuit to B+ P1369 - Cyl. 5, ignition circuit short to ground P1370 - Cyl. 6, ignition circuit Open Circuit P1371 - Cyl. 6, ignition circuit Short Circuit to B+ P1372 - Cyl. 6, ignition circuit short to ground P1373 - Cyl. 7, ignition circuit Open Circuit P1374 - Cyl. 7, ignition circuit Short Circuit to B+ P1375 - Cyl. 7, ignition circuit short to ground
7. P1376 - Cyl. 8, ignition circuit Open Circuit P1377 - Cyl. 8, ignition circuit Short Circuit to B+ P1378 - Cyl. 8, ignition circuit short to ground P1386 - Internal Control Module Knock Control Circ.Error P1387 - Internal Contr. Module altitude sensor error P1388 - Internal Contr. Module drive by wire error P1391 - Camshaft Pos.Sensor,Bank2 Short to Ground P1392 - Camshaft Pos.Sensor,Bank2 Open Circ./Short to B+ P1393 - Ignition Coil Power Output Stage 1 Electrical Malfunction P1394 - Ignition Coil Power Output Stage 2 Electrical Malfunction P1395 - Ignition Coil Power Output Stage 3 Electrical Malfunction P1396 - Engine Speed Sensor Missing Tooth P1397 - Engine speed wheel Adaptation limit reached P1398 - Engine RPM signal, TD Short to ground P1399 - Engine RPM signal, TD Short Circuit to B+ P1400 - EGR Valve Circ Electrical Malfunction P1401 - EGR Valve Circ Short to Ground P1402 - EGR Valve Circ Short to B+ P1403 - EGR Flow Deviation P1404 - EGR Flow Basic Setting not carried out P1406 - EGR Temp.Sensor Range/Performance P1407 - EGR Temp.Sensor Signal too Low P1408 - EGR Temp.Sensor Signal too High P1409 - Tank Ventilation Valve Circ. Electrical Malfunction P1410 - Tank Ventilation Valve Circ. Short to B+ P1411 - Sec.Air Inj.Sys.,Bank2 Flow too Flow P1412 - EGR Different.Pressure Sensor Signal too Low P1413 - EGR Different.Pressure Sensor Signal too High P1414 - Sec.Air Inj.Sys.,Bank2 Leak Detected P1417 - Fuel Level Sensor Circ Signal too Low P1418 - Fuel Level Sensor Circ Signal too High P1420 - Sec.Air Inj.Valve Circ Electrical Malfunction P1421 - Sec.Air Inj.Valve Circ Short to Ground P1422 - Sec.Air Inj.Sys.Contr.Valve Circ Short to B+
8. P1423 - Sec.Air Inj.Sys.,Bank1 Flow too Low P1424 - Sec.Air Inj.Sys.,Bank1 Leak Detected P1425 - Tank Vent.Valve Short to Ground P1426 - Tank Vent.Valve Open P1432 - Sec.Air Inj.Valve Open P1433 - Sec.Air Inj.Sys.Pump Relay Circ. open P1434 - Sec.Air Inj.Sys.Pump Relay Circ. Short to B+ P1435 - Sec.Air Inj.Sys.Pump Relay Circ. Short to ground P1436 - Sec.Air Inj.Sys.Pump Relay Circ. Electrical Malfunction P1439 - EGR Potentiometer Error in Basic Seting P1440 - EGR Valve Power Stage Open P1441 - EGR Valve Circ Open/Short to Ground P1442 - EGR Valve Position Sensor Signal too high P1443 - EGR Valve Position Sensor Signal too low P1444 - EGR Valve Position Sensor range/performance P1445 - Catalyst Temp.Sensor 2 Circ. Range/Performance P1446 - Catalyst Temp.Circ Short to Ground P1447 - Catalyst Temp.Circ Open/Short to B+ P1448 Catalyst Temp.Sensor 2 Circ. Short to Ground P1449 - Catalyst Temp.Sensor 2 Circ. Open/Short to B+ P1450 - Sec.Air Inj.Sys.Circ Short to B+ P1451 - Sec.Air Inj.Sys.Circ Short to Ground P1452 - Sec.Air Inj.Sys. Open Circ. P1453 - Exhaust gas temperature sensor 1 open/short to B+ P1454 - Exhaust gas temperature sensor short 1 to ground P1455 - Exhaust gas temperature sensor 1 range/performance P1456 - Exhaust gas temperature control bank 1 limit attained P1457 - Exhaust gas temperature sensor 2 open/short to B+ P1458 - Exhaust gas temperature sensor 2 short to ground P1459 - Exhaust gas temperature sensor 2 range/performance P1460 - Exhaust gas temperature control bank 2 limit attained P1461 - Exhaust gas temperature control bank 1 Range/Performance P1462 - Exhaust gas temperature control bank 2 Range/Performance P1465 - Additive Pump Short Circuit to B+
9. P1466 - Additive Pump Open/Short to Ground P1467 - EVAP Canister Purge Solenoid Valve Short Circuit to B+ P1468 - EVAP Canister Purge Solenoid Valve Short Circuit to Ground P1469 - EVAP Canister Purge Solenoid Valve Open Circuit P1470 - EVAP Emission Contr.LDP Circ Electrical Malfunction P1471 - EVAP Emission Contr.LDP Circ Short to B+ P1472 - EVAP Emission Contr.LDP Circ Short to Ground P1473 - EVAP Emission Contr.LDP Circ Open Circ. P1474 - EVAP Canister Purge Solenoid Valve electrical malfunction P1475 - EVAP Emission Contr.LDP Circ Malfunction/Signal Circ.Open P1476 - EVAP Emission Contr.LDP Circ Malfunction/Insufficient Vacuum P1477 - EVAP Emission Contr.LDP Circ Malfunction P1478 - EVAP Emission Contr.LDP Circ Clamped Tube Detected P1500 - Fuel Pump Relay Circ. Electrical Malfunction P1501 - Fuel Pump Relay Circ. Short to Ground P1502 - Fuel Pump Relay Circ. Short to B+ P1503 - Load signal from Alternator Term. DF Range/performance/Incorrect Signal P1504 - Intake Air Sys.Bypass Leak Detected P1505 - Closed Throttle Pos. Does Not Close/Open Circ P1506 - Closed Throttle Pos.Switch Does Not Open/Short to Ground P1507 - Idle Sys.Learned Value Lower Limit Attained P1508 - Idle Sys.Learned Value Upper Limit Attained P1509 - Idle Air Control Circ. Electrical Malfunction P1510 - Idle Air Control Circ. Short to B+ P1511 - Intake Manifold Changeover Valve circuit electrical malfunction P1512 - Intake Manifold Changeover Valve circuit Short to B+ P1513 - Intake Manifold Changeover Valve2 circuit Short to B+ P1514 - Intake Manifold Changeover Valve2 circuit Short to ground P1515 - Intake Manifold Changeover Valve circuit Short to Ground P1516 - Intake Manifold Changeover Valve circuit Open P1517 - Main Relay Circ. Electrical Malfunction P1518 - Main Relay Circ. Short to B+ P1519 - Intake Camshaft Contr.,Bank1 Malfunction P1520 - Intake Manifold Changeover Valve2 circuit Open
10. P1521 - Intake Manifold Changeover Valve2 circuit electrical malfunction P1522 - Intake Camshaft Contr.,Bank2 Malfunction P1523 - Crash Signal from Airbag Control Unit range/performance P1525 - Intake Camshaft Contr.Circ.,Bank1 Electrical Malfunction P1526 - Intake Camshaft Contr.Circ.,Bank1 Short to B+ P1527 - Intake Camshaft Contr.Circ.,Bank1 Short to Ground P1528 - Intake Camshaft Contr.Circ.,Bank1 Open P1529 - Camshaft Control Circuit Short to B+ P1530 - Camshaft Control Circuit Short to ground P1531 - Camshaft Control Circuit open P1533 - Intake Camshaft Contr.Circ.,Bank2 Electrical Malfunction P1534 - Intake Camshaft Contr.Circ.,Bank2 Short to B+ P1535 - Intake Camshaft Contr.Circ.,Bank2 Short to Ground P1536 - Intake Camshaft Contr.Circ.,Bank2 Open P1537 - Engine Shutoff Solenoid Malfunction P1538 - Engine Shutoff Solenoid Open/Short to Ground P1539 - Clutch Vacuum Vent Valve Switch Incorrect signal P1540 - Vehicle Speed Sensor High Input P1541 - Fuel Pump Relay Circ Open P1542 - Throttle Actuation Potentiometer Range/Performance P1543 - Throttle Actuation Potentiometer Signal too Low P1544 - Throttle Actuation Potentiometer Signal too High P1545 - Throttle Pos.Contr Malfunction P1546 - Boost Pressure Contr.Valve Short to B+ P1547 - Boost Pressure Contr.Valve Short to Ground P1548 - Boost Pressure Contr.Valve Open P1549 - Boost Pressure Contr.Valve Short to Ground P1550 - Charge Pressure Deviation P1551 - Barometric Pressure Sensor Circ. Short to B+ P1552 - Barometric Pressure Sensor Circ. Open/Short to Ground P1553 - Barometric/manifold pressure signal ratio out of range P1554 - Idle Speed Contr.Throttle Pos. Basic Setting Conditions not met P1555 - Charge Pressure Upper Limit exceeded P1556 - Charge Pressure Contr. Negative Deviation
11. P1557 - Charge Pressure Contr. Positive Deviation P1558 - Throttle Actuator Electrical Malfunction P1559 - Idle Speed Contr.Throttle Pos. Adaptation Malfunction P1560 - Maximum Engine Speed Exceeded P1561 - Quantity Adjuster Deviation P1562 - Quantity Adjuster Upper Limit Attained P1563 - Quantity Adjuster Lower Limit Attained P1564 - Idle Speed Contr.Throttle Pos. Low Voltage During Adaptation P1565 - Idle Speed Control Throttle Position lower limit not attained P1566 - Load signal from A/C compressor range/performance P1567 - Load signal from A/C compressor no signal P1568 - Idle Speed Contr.Throttle Pos. mechanical Malfunction P1569 - Cruise control switch Incorrect signal P1570 - Contr.Module Locked P1571 - Left Eng. Mount Solenoid Valve Short to B+ P1572 - Left Eng. Mount Solenoid Valve Short to ground P1573 - Left Eng. Mount Solenoid Valve Open circuit P1574 - Left Eng. Mount Solenoid Valve Electrical fault in circuit P1575 - Right Eng. Mount Solenoid Valve Short to B+ P1576 - Right Eng. Mount Solenoid Valve Short to ground P1577 - Right Eng. Mount Solenoid Valve Open circuit P1578 - Right Eng. Mount Solenoid Valve Electrical fault in circuit P1579 - Idle Speed Contr.Throttle Pos. Adaptation not started P1580 - Throttle Actuator B1 Malfunction P1581 - Idle Speed Contr.Throttle Pos. Basic Setting Not Carried Out P1582 - Idle Adaptation at Limit P1583 - Transmission mount valves Short to B+ P1584 - Transmission mount valves Short to ground P1585 - Transmission mount valves Open circuit P1586 - Engine mount solenoid valves Short to B+ P1587 - Engine mount solenoid valves Short to ground P1588 - Engine mount solenoid valves Open circuit P1600 - Power Supply (B+) Terminal 15 Low Voltage P1602 - Power Supply (B+) Terminal 30 Low Voltage
12. P1603 - Internal Control Module Malfunction P1604 - Internal Control Module Driver Error P1605 - Rough Road/Acceleration Sensor Electrical Malfunction P1606 - Rough Road Spec Engine Torque ABS-ECU Electrical Malfunction P1607 - Vehicle speed signal Error message from instrument cluster P1608 - Steering angle signal Error message from steering angle sensor P1609 - Crash shut-down activated P1611 - MIL Call-up Circ./Transm.Contr.Module Short to Ground P1612 - Electronic Control Module Incorrect Coding P1613 - MIL Call-up Circ Open/Short to B+ P1614 - MIL Call-up Circ./Transm.Contr.Module Range/Performance P1615 - Engine Oil Temperature Sensor Circuit range/performance P1616 - Glow Plug/Heater Indicator Circ. Short to B+ P1617 - Glow Plug/Heater Indicator Circ. Open/Short to Ground P1618 - Glow Plug/Heater Relay Circ. Short to B+ P1619 - Glow Plug/Heater Relay Circ. Open/Short to Ground P1620 - Engine coolant temperature signal open/short to B+ P1621 - Engine coolant temperature signal short to ground P1622 - Engine coolant temperature signal range/performance P1623 - Data Bus Powertrain No Communication P1624 - MIL Request Sign.active P1625 - Data-Bus Powertrain Unplausible Message from Transm.Contr. P1626 - Data-Bus Powertrain Missing Message from Transm.Contr. P1627 - Data-Bus Powertrain missing message from fuel injection pump P1628 - Data-Bus Powertrain missing message from steering sensor P1629 - Data-Bus Powertrain missing message from distance control P1630 - Accelera.Pedal Pos.Sensor 1 Signal too Low P1631 - Accelera.Pedal Pos.Sensor 1 Signal too High P1632 - Accelera.Pedal Pos.Sensor 1 Power Supply Malfunction P1633 - Accelera.Pedal Pos.Sensor 2 Signal too Low P1634 - Accelera.Pedal Pos.Sensor 2 Signal too High P1635 - Data Bus Powertrain missing message f.air condition control P1636 - Data Bus Powertrain missing message from Airbag control P1637 - Data Bus Powertrain missing message f.central electr.control
13. P1638 - Data Bus Powertrain missing message from clutch control P1639 - Accelera.Pedal Pos.Sensor 1+2 Range/Performance P1640 - Internal Contr.Module (EEPROM) Error P1641 - Please check DTC Memory of Air Condition ECU P1642 - Please check DTC Memory of Airbag ECU P1643 - Please check DTC Memory of central electric ECU P1644 - Please check DTC Memory of clutch ECU P1645 - Data Bus Powertrain missing message f.all wheel drive contr. P1646 - Please Check DTC Memory of all wheel drive ECU P1647 - Please check coding of ECUs in Data Bus Powertrain P1648 - Data Bus Powertrain Malfunction P1649 - Data Bus Powertrain Missing message from ABS Control Module P1650 - Data Bus Powertrain Missing message fr.instrument panel ECU P1651 - Data Bus Powertrain missing messages P1652 - Please check DTC Memory of transmission ECU P1653 - Please check DTC Memory of ABS Control Module P1654 - Please check DTC Memory of control panel ECU P1655 - Please check DTC Memory of ADR Control Module P1656 - A/C clutch relay circuit short to ground P1657 - A/C clutch relay circuit short to B+ P1658 - Data Bus Powertrain Incorrect signal from ADR Control Module P1676 - Drive by Wire-MIL Circ. Electrical Malfunction P1677 - Drive by Wire-MIL Circ. Short to B+ P1678 - Drive by Wire-MIL Circ. Short to Ground P1679 - Drive by Wire-MIL Circ. Open P1681 - Contr.Unit Programming, Programming not Finished P1684 - Contr.Unit Programming Communication Error P1686 - Contr.Unit Error Programming Error P1690 - Malfunction Indication Light Malfunction P1691 - Malfunction Indication Light Open P1692 - Malfunction Indication Light Short to Ground P1693 - Malfunction Indication Light Short to B+ P1694 - Malfunction Indication Light Open/Short to Ground P1704 - Kick Down Switch Malfunction
14. P1705 - Gear/Ratio Monitoring Adaptation limit reached P1711 - Wheel Speed Signal 1 Range/Performance P1716 - Wheel Speed Signal 2 Range/Performance P1721 - Wheel Speed Signal 3 Range/Performance P1723 - Starter Interlock Circ. Open P1724 - Starter Interlock Circ. Short to Ground P1726 - Wheel Speed Signal 4 Range/Performance P1728 - Different Wheel Speed Signals Range/Performance P1729 - Starter Interlock Circ. Short to B+ P1733 - Tiptronic Switch Down Circ. Short to Ground P1739 - Tiptronic Switch up Circ. Short to Ground P1740 - Clutch temperature control P1741 - Clutch pressure adaptation at limit P1742 - Clutch torque adaptation at limit P1743 - Clutch slip control signal too high P1744 - Tiptronic Switch Recognition Circ. Short to Ground P1745 - Transm.Contr.Unit Relay Short to B+ P1746 - Transm.Contr.Unit Relay Malfunction P1747 - Transm.Contr.Unit Relay Open/Short to Ground P1748 - Transm.Contr.Unit Self-Check P1749 - Transm.Contr.Unit Incorrect Coded P1750 - Power Supply Voltage Low Voltage P1751 - Power Supply Voltage High Voltage P1752 - Power Supply Malfunction P1760 - Shift Lock Malfunction P1761 - Shift Lock Short to Ground P1762 - Shift Lock Short to B+ P1763 - Shift Lock Open P1764 - Transmission temperature control P1765 - Hydraulic Pressure Sensor 2 adaptation at limit P1766 - Throttle Angle Signal Stuck Off P1767 - Throttle Angle Signal Stuck On P1768 - Hydraulic Pressure Sensor 2 Too High P1769 - Hydraulic Pressure Sensor 2 Too Low
15. P1770 - Load Signal Range/Performance P1771 - Load Signal Stuck Off P1772 - Load Signal Stuck On P1773 - Hydraulic Pressure Sensor 1 Too High P1774 - Hydraulic Pressure Sensor 1 Too Low P1775 - Hydraulic Pressure Sensor 1 adaptation at limit P1776 - Hydraulic Pressure Sensor 1 range/performance P1777 - Hydraulic Pressure Sensor 2 range/performance P1778 - Solenoid EV7 Electrical Malfunction P1781 - Engine Torque Reduction Open/Short to Ground P1782 - Engine Torque Reduction Short to B+ P1784 - Shift up/down Wire Open/Short to Ground P1785 - Shift up/down Wire Short to B+ P1786 - Reversing Light Circ. Open P1787 - Reversing Light Circ. Short to Ground P1788 - Reversing Light Circ. Short to B+ P1789 - Idle Speed Intervention Circ. Error Message from Engine Contr. P1790 - Transmission Range Display Circ. Open P1791 - Transmission Range Display Circ. Short to Ground P1792 - Transmission Range Display Circ. Short to B+ P1793 - Output Speed Sensor 2 Circ. No Signal P1795 - Vehicle Speed Signal Circ. Open P1796 - Vehicle Speed Signal Circ. Short to Ground P1797 - Vehicle Speed Signal Circ. Short to B+ P1798 - Output Speed Sensor 2 Circ. Range/Performance P1799 - Output Speed Sensor 2 Circ. Rpm too High P1813 - Pressure Contr.Solenoid 1 Electrical P1814 - Pressure Contr.Solenoid 1 Open/Short to Ground P1815 - Pressure Contr.Solenoid 1 Short to B+ P1818 - Pressure Contr.Solenoid 2 Electrical P1819 - Pressure Contr.Solenoid 2 Open/Short to Ground P1820 - Pressure Contr.Solenoid 2 Short to B+ P1823 - Pressure Contr.Solenoid 3 Electrical P1824 - Pressure Contr.Solenoid 3 Open/Short to Ground
16. P1825 - Pressure Contr.Solenoid 3 Short to B+ P1828 - Pressure Contr.Solenoid 4 Electrical P1829 - Pressure Contr.Solenoid 4 Open/Short to Ground P1830 - Pressure Contr.Solenoid 4 Short to B+ P1834 - Pressure Contr.Solenoid 5 Open/Short to Ground P1835 - Pressure Contr.Solenoid 5 Short to B+ P1841 - Engine/Transmission Control Modules Versions do not match P1842 - Please check DTC Memory of instrument panel ECU P1843 - Please check DTC Memory of ADR Control Module P1844 - Please check DTC Memory of central electric control ECU P1847 - Please check DTC Memory of brake system ECU P1848 - Please check DTC Memory of engine ECU P1849 - Please check DTC Memory of transmission ECU P1850 - Data-Bus Powertrain Missing Message from Engine Contr. P1851 - Data-Bus Powertrain Missing Message from Brake Contr. P1852 - Data-Bus Powertrain Unplausible Message from Engine Contr. P1853 - Data-Bus Powertrain Unplausible Message from Brake Contr. P1854 - Data-Bus Powertrain Hardware Defective P1855 - Data-Bus Powertrain Software version Contr. P1856 - Throttle/Pedal Pos.Sensor A Circ. Error Message from Engine Contr. P1857 - Load Signal Error Message from Engine Contr. P1858 - Engine Speed Input Circ. Error Message from Engine Contr. P1859 - Brake Switch Circ. Error Message from Engine Contr. P1860 - Kick Down Switch Error Message from Engine Contr. P1861 - Throttle Position (TP) sensor Error Message from ECM P1862 - Data Bus Powertrain Missing message from instr. panel ECU P1863 - Data Bus Powertrain Missing Message from St. Angle Sensor P1864 - Data Bus Powertrain Missing message from ADR control module P1865 - Data Bus Powertrain Missing message from central electronics P1866 - Data Bus Powertrain Missing messages 
