dot-obdgpslogger(5)

NAME
dot-obdgpslogger - configuration file for obdgpslogger

DESCRIPTION
Configuration file for obdgpslogger Comments Any line whose first non-whitespace character is a # is a comment obddevice=<string> Full path to obd device entry [typically /dev/something] gpsdevice=<string> Full path to gps device entry [typically /dev/something] log_columns=<string> Command-separated list of db_column entries to log. These are probably things you want to draw from "obdgpslogger -p" log_file=<string> Write to this logfile. Can be relative or absolute path samplerate=<integer> Number of samples to take per second. 0 for "as fast as you can" baudrate=<integer> Set serial port baudrate to this. -1 disables attempt to change, or 0 to let the software try to guess. baudrate_upgrade=<integer> Upgrade the baudrate to this after successful setup. -1 disables attempt to change, or 0 to let the software try to figure out the best choice. optimisations=<integer> Set to 1 to enable ELM optimisations

FILES TO PARSE
The system loads these files, in order. Each one overwrites any settings from the file before it:

1) /etc/obdgpslogger

2) $HOME/.obdgpslogger

3) /var/run/obdftdipty.device

4) getenv("OBD_CONFIGFILE")

ENVIRONMENT VARIABLES

OBD_CONFIGFILE
    Full path to the obd config file you wish to read

HOME
    If set, read .obdgpslogger from this dir

APPDATA
    If HOME isn't set, will attempt to read .obdgpslogger from here instead

SEE ALSO
obdgpslogger(1), obdgui(1)

AUTHORS
Gary "Chunky Ks" Briggs <chunky@icculus.org>